[index] AT-AR3050S/AT-AR4050S/AT-AR4050S-5G コマンドリファレンス 5.5.4

# show wireless ap

モード: 非特権EXECモード
カテゴリー: 無線LANコントローラー（AWC対応） / AP個別設定（AP登録）

`> show wireless ap [<1-65535>|all] [brief|status|detail]`

管理下APの登録情報を表示する。

### パラメーター

`<1-65535>` | AP登録番号。カンマ、ハイフン区切りで複数指定が可能。本パラメーター指定時は指定したAPの登録情報だけを表示する。省略時はallを指定したのと同じ動作となる
`all` | すべてのAP登録情報を表示する（省略時動作）
`brief` | AP登録情報を簡潔に表示させたいときに指定する。省略時は詳細な情報が表示される
`status` | APのステータスを表示する
`detail` | APの詳細なステータスとデバイス情報を表示する

### 使用例

    awplus> show wireless ap 1 ↓
    AP ID 1:
     Status ........................ Enable
     Description ...................
     AP Profile .................... 1
     IP Address .................... 192.168.1.101
     MAC Address ................... 0000.5e00.5301
     Login Username ................
     Login Password ................
     Radio 1:
      OverrideRadioStatus ..........
      Channel ...................... auto
      Power ........................ auto
     Radio 2:
      OverrideRadioStatus ..........
      Channel ...................... auto
      Power ........................ auto

    awplus> show wireless ap brief ↓
    ID    Description Status  Prof  IP Address      MAC Address
    ----- ----------- ------- ----- --------------- --------------
        1             Enable      1 192.168.1.101   0000.5e00.5301
        2             Enable      1 192.168.1.102   0000.5e00.5302
        3             Enable      2 192.168.1.103   0000.5e00.5303

    awplus> show wireless ap status ↓
    ID    Model           FW ver     Manage rupt Config   c Clnt Uptime
    ----- --------------- ---------- ----------- ---------- ---- ---------------
        1 AT-TQ5403       X.X.X-X.X  Managd ---- Succeed  -    0          848048
        2 AT-TQ6602       X.X.X-X.X  Managd ---- Succeed  -    0          520317
        3 AT-TQ6602 GEN2  X.X.X-X.X  Managd ---- Succeed  -    0           65556
        4 AT-TQ6702 GEN2  X.X.X-X.X  Managd ---- Succeed  -    0          161036

     Legends:
     - ID     ... ID of Access Point entry
     - Model  ... Model name of Access Point
     - FW ver ... Firmware version of Access Point
     - Manage ... Management Status of Access Point
                     Managd: Managed
                     Discvd: Discovered
                     Joined: Joinded
                     Failed: Failed
                     Reboot: Rebooting
                     Update: Updating
     - r      ... Reboot Status
                     R: Requested
                     *: Rebooting
                     S: Succeeded
                     F: Failed
     - u      ... Update Status
                     R: Requested
                     *: Upgrading
                     S: Succeeded
                     F: Failed
     - p      ... Power-Channel Status
                     R: Requested
                     S: Succeeded
                     F: Failed
     - t      ... Technical support file collectiong Status
                     R: Requested
                     E: Executing
                     S: Succeeded
                     F: Failed (includes aborted)
     - Config ... Configuration Status
                     NotConfg: Not Configured
                     InProgrs: In Progress
                     Succeed : Succeeded
                     Failed  : Failed
                     Unknown : Unknown
     - c      ... Configuration Apply Status
                     R: Requested
                     A: Applying
                     S: Succeeded
                     F: Failed
     - Clnt   ... Number of connected clients
     - Uptime ... Uptime in seconds

    awplus> show wireless ap detail ↓
    AP ID 1:
     Description ................... TQ5403
     AP Profile .................... 3
     IP Address .................... 192.168.x.x
     MAC Address ................... XXXX.XXXX.XXXX
     Model ......................... AT-TQ5403
     Serial ........................
     Firmware Version .............. X.X.X-X.X
     Management Status ............. Joined
     Configuration Status .......... In Progress (Modified)
     Crash Log Status .............. -
     Clients........................ 0
     Sysup time..................... 0
     Operational Status:
      Reboot Status ................. -
      Firmware Upgrade Status ....... -
      Configuration Apply Status .... -
      Auto Channel Power Status ..... -
     Radio 1:
      Channel ...................... 5
      Power ........................ 10
      Radar detection .............. None
     Radio 2:
      Channel ...................... 40
      Power ........................ 100
      Radar detection .............. None

### 注意・補足事項

■ 登録したAPの数が管理可能数を超えても、show wireless apコマンドの表示上は管理対象になっているAPとなっていないAPの区別ができない。管理可能数を超える数のAPを登録する場合は、実際に管理対象とするAPの登録のみをAP登録モードのenableコマンドで有効化し、それ以外のAPは同コマンドで無効化すること。なお、登録AP数が管理可能数を超えている場合は、AP登録番号の小さいものが優先的に管理対象となる。

### 関連コマンド

ap（無線LANコントローラーモード）

(C) 2015 - 2024 アライドテレシスホールディングス株式会社

PN: 613-002107 Rev.BC