[index] AT-AR3050S/AT-AR4050S/AT-AR4050S-5G コマンドリファレンス 5.5.4

# show log config

モード: 特権EXECモード
カテゴリー: 運用・管理 / ログ

`# show log config`

ログ出力先の定義内容（出力先、状態、メッセージフィルターなど）や統計情報を表示する。

### 使用例

    awplus# show log config ↓

    Facility: local0 (local use 0)

    Buffered log:
      Status ......... enabled
      Maximum size ... 50kb
      Filters:
     *1   Level ...... notices
          Program .... any
          Facility ... any
          Msg text ... any
          Type ....... include
      Statistics ..... 59 messages received, 20 accepted by filter (2012 Jan 13 23:3
    3:17)
    Permanent log:
      Status ......... enabled
      Maximum size ... 50kb
      Filters:
     *1   Level ...... warnings
          Program .... any
          Facility ... any
          Msg text ... any
          Type ....... include
      Statistics ..... 59 messages received, 0 accepted by filter (2012 Jan 13 23:33
    :17)
    Host 10.100.10.100:
      Time offset .... +3:00
      Offset type .... Local
      Source ......... 192.168.1.100
      Secured ........ disabled
      Delay parameters:
        Startup-Delay: 120
        Buffered-Messages: 2000
      Filters:
      1   Level ...... errors
          Program .... any
          Facility ... any
          Msg text ... any
          Type ....... include
      2   Level ...... any
          Program .... ospf
          Facility ... any
          Msg text ... any
          Type ....... include
      Statistics ..... 59 messages received, 1 accepted by filter (2012 Jan 13 23:33
    :17)
    Monitor log:
      Filters:
     *1   Level ...... debugging
          Program .... any
          Facility ... any
          Msg text ... any
          Type ....... include
      Statistics ..... Not available
    Console log:
      Status ......... enabled
      List of consoles:
      1 .............. ttyS0
      Filters:
     *1   Level ...... critical
          Program .... any
          Facility ... any
          Msg text ... any
          Type ....... include
      Statistics ..... 59 messages received, 0 accepted (2012 Jan 13 23:33:17)
    External log:
      Status ......... enabled
      Log file ....... usb:/sample.log
      Rotation ....... 4
      Maximum size ... 1024kb
      Filters:
     *1   Level ...... notices
          Program .... any
          Facility ... any
          Msg text ... any
          Type ....... include
      Statistics ..... 225960 messages received, 219939 accepted, 0 excluded (2017 J
    un 19 03:04:18 sysl)

### 注意・補足事項

■ 本コマンドはEXECモードだけでなくグローバルコンフィグモードでも実行できる。

### 関連コマンド

ip vrf（グローバルコンフィグモード）
log（グローバルコンフィグモード）
log exclude（グローバルコンフィグモード）
log facility（グローバルコンフィグモード）
log host source（グローバルコンフィグモード）
log host startup-delay（グローバルコンフィグモード）
log rotate（グローバルコンフィグモード）
log size（グローバルコンフィグモード）
log time（グローバルコンフィグモード）
log(filter)（グローバルコンフィグモード）

(C) 2015 - 2024 アライドテレシスホールディングス株式会社

PN: 613-002107 Rev.BC