[index] AT-AR3050S/AT-AR4050S/AT-AR4050S-5G コマンドリファレンス 5.5.4

# show 5g status

モード: 非特権EXECモード
カテゴリー: インターフェース / ワイヤレスWAN

`> show 5g status`

内蔵ワイヤレスWANモジュールの状態を表示する。

### 使用例

    awplus> show 5g status ↓
    Modem:
        Sierra Wireless, Incorporated
        EM9191 (355890340105928)
        Revision: 1
        SWIX55C_02.08.01.00 58f60e jenkins 2021/03/12 18:05:48
        Radio is enabled

    Status:
    Current Time:  159574           Temperature: 38
    Modem Mitigate Level: 0         ModemProc Mitigate Level: 0
    Reset Counter: 1                Mode:        ONLINE
    System mode:   ENDC             PS state:    Attached
    LTE band:      B3               LTE bw:      20 MHz
    LTE Rx chan:   1850             LTE Tx chan: 19850
    LTE SSC1 state:INACTIVE         LTE SSC1 band: B1
    LTE SSC1 bw  : 15 MHz           LTE SSC1 chan: 276
    LTE SSC2 state:INACTIVE         LTE SSC2 band: B19
    LTE SSC2 bw  : 10 MHz           LTE SSC2 chan: 6100
    EMM state:     Registered       Normal Service
    RRC state:     RRC Connected
    IMS reg state: UNKNOWN          IMS mode:    Not Support
    IMS Srv State: UNKNOWN SMS,UNKNOWN VoIP

    PCC RxM RSSI:  -53              PCC RxM RSRP:  -82
    PCC RxD RSSI:  -55              PCC RxD RSRP:  -82
    PCC RxM1 RSSI:  -51             PCC RxM1 RSRP:  -81
    PCC RxD1 RSSI:  -52             PCC RxD1 RSRP:  -82
    SCC1 RxM RSSI: -70              SCC1 RxM RSRP: -94
    SCC1 RxD RSSI: -67              SCC1 RxD RSRP: -89
    SCC1 RxM1 RSSI:  ---            SCC1 RxM1 RSRP:  ---
    SCC1 RxD1 RSSI:  ---            SCC1 RxD1 RSRP:  ---
    SCC2 RxM RSSI: -58              SCC2 RxM RSRP: -81
    SCC2 RxD RSSI: -59              SCC2 RxD RSRP: -80
    Tx Power:      3                TAC:         1669 (5737)
    RSRQ (dB):     -10.1            Cell ID:     02cede51 (47111761)
    SINR (dB):      3.2
    NR Tx Power:      11
    NR5G band:       No band        NR5G bw:         5 MHz
    NR5G Rx chan:    703334         NR5G Tx chan:    703334
    NR5G RSRP (dBm): -115           NR5G RSRQ (dB):  -13
    NR5G SINR (dB):   3.0

    Power Supply:
    Volt state: Normal
    Power supply voltage: 3310 mV (ADC: 17006)

    Power Control:
    State: Online
    LPM voters - Temp:0, Volt:0, User:0, W_DISABLE:0, IMSWITCH:0, BIOS:0, LWM2M:0, OMADM:0, FOTA:0, RFCAL:0
    LPM persistence - None

    5G NR Info:
    Connectivity Mode: NSA

    Cell ID:         81
    NR5G band:       No band                Carrier Index:   0
    NR5G dl bw:      5 MHz                  NR5G ul bw:      Unknown
    NR5G Rx chan:    703334                 NR5G Tx chan:    703334
    NR5G dl MIMO:    0                      NR5G ul MIMO:    1
    NR5G(sub6) RxM RSSI (dBm):   -77.5      NR5G(sub6) RxD RSSI (dBm):   -79.9
    NR5G(sub6) RxM1 RSSI (dBm):  -77.0      NR5G(sub6) RxD1 RSSI (dBm):  -81.3

    NR5G RSRP (dBm): -115                   NR5G RSRQ (dB):  -13
    NR5G SINR (dB):   3.0

### 注意・補足事項

■ 本コマンドはAT-AR4050S-5Gでのみ有効。

(C) 2015 - 2024 アライドテレシスホールディングス株式会社

PN: 613-002107 Rev.BC