[index] CentreCOM AR550S コマンドリファレンス 2.9

# SHOW BGP MEMLIMIT SCAN

カテゴリー：IP / 経路制御（BGP-4）

`SHOW BGP MEMLIMIT SCAN`

BGPモジュールのメモリー容量の情報を表示する。

入力・出力・画面例

    Manager > show bgp memlimit scan

    BGP Memory Limit: 85%, Actual Use: 57%
    Module Freelist Stats: moduleId = 5
    module buffer use: 18686
    module percent use: 34%
          list          unitSize  freeUsed  buffersUsed
    -------------------------------------------------
          00f33c6c      84        0         0
          00f46b6c      12        0         0
          00f46024      88        0         0
          00f33b04      68        0         0
          00f33c9c      48        104874    4996
          00f46c78      12        0         0
          00f4f0fc      32        196984    6156
          00f557e4      236       104874    26220
    -------------------------------------------------
    Module Freelist Stats: moduleId = 103
    module buffer use: 31011
    module percent use: 57%
    list unitSize freeUsed buffersUsed
    -------------------------------------------------
          00d0caf4      24        0         0
          00d0ca94      12        0         0
          00d0cc40      32        0         0
          00d0cff4      32        0         0
          00d0ccc8      8         155       1
          00d0ca64      512       0         0
          00d0cbb0      8         0         0
          00d0cf14      8         19439     76
          00d0cc10      8         0         0
          00d0c7e0      64        21643     677
          00d0cbe0      524       0         0
          00d0cf9c      116       180       11
          00d0cdf8      36        19262     338
          00d0c810      20        0         0
          00d0ce28      16        0         0
          00d0cf44      52        196980    5051
          00d0cc98      40        314616    6169
          00d0bc88      20        0         0
          00d0d024      20        0         0
          00d0b860      40        2         1
          00d0bc58      1012      2         1
          00d0d07c      40        0         0
          00d0cac4      16        0         0
          00f33c6c      84        0         0
          00f46b6c      12        0         0
          00f46024      88        0         0
          00f33b04      68        0         0
          00f33c9c      48        104874    4996
          00f46c78      12        0         0
          00f4f0fc      32        196984    6156
          00f557e4      236       104874    26220
    -------------------------------------------------

関連コマンド

SET BGP BACKOFF
SET BGP MEMLIMIT
SHOW BGP MEMLIMIT

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2439, BGP Route Flap Damping
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H