## CentreCOM AR550S 設定例集 2.9
##  161 CUGサービスを利用した3拠点間L2TP接続（インターネット接続はセンタールーター経由）
##  ルーターCのコンフィグ

ENABLE L2TP 
ENABLE L2TP SERVER=BOTH 
ADD L2TP PASSWORD=l2tpC
ADD L2TP CALL=remote2 REMOTE=remote2 TYPE=VIRTUAL IP=172.16.0.1 PRECEDENCE=OUT PASSWORD=l2tpA 
CREATE PPP=0 OVER=eth0-ANY
SET PPP=0 OVER=eth0-ANY BAP=OFF IPREQUEST=ON USER=userC@cug PASSWORD=cugpasswdC LQR=OFF ECHO=ON
CREATE PPP=12 OVER=TNL-remote2 IDLE=ON BAP=OFF LQR=OFF
ENABLE IP
ENABLE IP REMOTEASSIGN
ADD IP INT=vlan1 IP=192.168.30.1 MASK=255.255.255.0
ADD IP INT=ppp0 IP=0.0.0.0
ADD IP INT=ppp12 IP=0.0.0.0
ADD IP ROUTE=172.16.0.1 MASK=255.255.255.255 INTERFACE=ppp0 NEXTHOP=0.0.0.0
ADD IP ROUTE=0.0.0.0 INT=ppp12 NEXTHOP=0.0.0.0 
ENABLE FIREWALL
CREATE FIREWALL POLICY=net
ENABLE FIREWALL POLICY=net ICMP_FORWARDING=PING,UNREACH
DISABLE FIREWALL POLICY=net IDENTPROXY
ADD FIREWALL POLICY=net INTERFACE=vlan1 TYPE=PRIVATE 
ADD FIREWALL POLICY=net INTERFACE=ppp0 TYPE=PUBLIC 
ADD FIREWALL POLICY=net INTERFACE=ppp12 TYPE=PRIVATE 
ADD FIREWALL POLICY=net RU=1 AC=ALLOW INT=ppp0 PROT=UDP PORT=1701 IP=172.16.0.3
