## CentreCOM AR550S 設定例集 2.9
##  146 WANロードバランス機能によるトラフィック負荷分散（Round Robinモード）
##  ルーターのコンフィグ

CREATE PPP=0 OVER=eth0-ANY
SET PPP=0 OVER=eth0-ANY BAP=OFF IPREQUEST=ON USER=user@ispA PASSWORD=isppasswdA LQR=OFF ECHO=ON
CREATE PPP=1 OVER=eth1-ANY
SET PPP=1 OVER=eth1-ANY BAP=OFF IPREQUEST=ON USER=user@ispB PASSWORD=isppasswdB LQR=OFF ECHO=ON
ENABLE IP
ENABLE IP REMOTEASSIGN
ADD IP INT=vlan1 IP=192.168.10.1 MASK=255.255.255.0
ADD IP INT=ppp0 IP=0.0.0.0
ADD IP INT=ppp1 IP=0.0.0.0
ADD IP ROUTE=0.0.0.0 INT=ppp0 NEXTHOP=0.0.0.0
ADD IP ROUTE=0.0.0.0 INT=ppp1 NEXTHOP=0.0.0.0
ENABLE FIREWALL
CREATE FIREWALL POLICY=net
ENABLE FIREWALL POLICY=net ICMP_F=PING,UNREACH
DISABLE FIREWALL POLICY=net IDENTPROXY
ADD FIREWALL POLICY=net INT=vlan1 TYPE=PRIVATE
ADD FIREWALL POLICY=net INT=ppp0 TYPE=PUBLIC
ADD FIREWALL POLICY=net INT=ppp1 TYPE=PUBLIC
ADD FIREWALL POLICY=net NAT=ENHANCED INT=vlan1 GBLINT=ppp0
ADD FIREWALL POLICY=net NAT=ENHANCED INT=vlan1 GBLINT=ppp1
DISABLE IP ROUTE MULTIPATH
ENABLE WANLB
ADD WANLB RESOURCE=ppp0
ADD WANLB RESOURCE=ppp1
