## CentreCOM AR550S 設定例集 2.9
##  50 PPPoEによるLAN型インターネット接続（DMZ）
##  ルーターのコンフィグ

CREATE PPP=0 OVER=eth0-ANY
SET PPP=0 OVER=eth0-ANY BAP=OFF IPREQUEST=ON USER=user@isp PASSWORD=isppasswd LQR=OFF ECHO=ON
ENABLE IP
ENABLE IP REMOTEASSIGN
ADD IP INT=eth1 IP=4.4.4.1 MASK=255.255.255.248
ADD IP INT=vlan1 IP=192.168.10.1 MASK=255.255.255.0
ADD IP INT=ppp0 IP=0.0.0.0
ADD IP ROUTE=0.0.0.0 INT=ppp0 NEXTHOP=0.0.0.0
ENABLE FIREWALL
CREATE FIREWALL POLICY=net
ENABLE FIREWALL POLICY=net ICMP_F=PING,UNREACH
DISABLE FIREWALL POLICY=net IDENTPROXY
ADD FIREWALL POLICY=net INT=eth1 TYPE=PRIVATE
ADD FIREWALL POLICY=net INT=vlan1 TYPE=PRIVATE
ADD FIREWALL POLICY=net INT=ppp0 TYPE=PUBLIC
ADD FIREWALL POLICY=net NAT=ENHANCED INT=vlan1 GBLINT=ppp0 GBLIP=4.4.4.1
ADD FIREWALL POLICY=net RULE=1 AC=ALLOW INT=ppp0 PROTO=TCP IP=4.4.4.2 PORT=80
ADD FIREWALL POLICY=net RULE=2 AC=ALLOW INT=ppp0 PROTO=TCP IP=4.4.4.3 PORT=25
ADD FIREWALL POLICY=net RULE=3 AC=ALLOW INT=ppp0 PROTO=TCP IP=4.4.4.4 PORT=53
ADD FIREWALL POLICY=net RULE=4 AC=ALLOW INT=ppp0 PROTO=UDP IP=4.4.4.4 PORT=53
