[index] CentreCOM AR550S コマンドリファレンス 2.9

# SHOW PPP

カテゴリー：PPP / PPPインターフェース

`SHOW PPP[=ppp-interface]`

ppp-interface: PPPインターフェース番号（0〜511）

PPPインターフェースに関する情報を表示する。

パラメーター

PPP: PPPインターフェース番号

入力・出力・画面例

    Manager bulbul> show ppp

      Name            Enabled  ifIndex  Over                  CP           State
      -----------------------------------------------------------------------------
      ppp0              YES      09                           IPCP         OPENED
                                        eth0-any              LCP          OPENED
      ppp1              YES      10                           IPCP         OPENED
                                        eth0-any              LCP          OPENED
      -----------------------------------------------------------------------------

表 1
Name | PPPインターフェース名
Enabled | インターフェースが有効（Enable）かどうか
ifIndex | MIB-IIオブジェクトifIndexの値
Over | 物理インターフェース名
CP | コントロールプロトコル名
State | 各コントロールプロトコルの状態（INITIAL、STARTING、CLOSED、STOPPED、CLOSING、STOPPING、REQ SENT、ACK RCVD、ACK SENT、OPENED）

関連コマンド

SHOW PPP CONFIG
SHOW PPP COUNTER

参考

RFC1331, The Point-to-Point Protocol (PPP) for the Transmission of Multi-protocol Datagrams over Point-to-Point Links
RFC1332, The PPP Internet Protocol Control Protocol (IPCP)
RFC1333, PPP Link Quality Monitoring
RFC1334, PPP Authentication Protocols
RFC1548, The Point-to-Point Protocol (PPP)
RFC1549, PPP in HDLC Framing
RFC1570, PPP LCP Extensions
RFC1638, PPP Bridging Control Protocol (BCP)
RFC1661, The Point-to-Point Protocol (PPP)
RFC1662, PPP in HDLC-like Framing
RFC1877, PPP Internet Protocol Control Protocol Extensions for Name Server Addresses
RFC2516, A Method for Transmitting PPP Over Ethernet (PPPoE)

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H