[index] CentreCOM AR550S コマンドリファレンス 2.9

# SHOW PRI COUNTER

カテゴリー：インターフェース / PRIインターフェース

`SHOW PRI[=pri-interface] COUNTER[={DIAGNOSTIC|INTERFACE|LINK|PRI}] [CHANNEL=channel] [HISTORY[=1..96]] [{NEAR|FAR|BOTH}]`

pri-interface: PRIインターフェース番号
channel: チャンネル番号（0〜31またはD）

PRIインターフェースのMIBカウンターを表示する。

パラメーター

PRI: PRIインターフェース番号。省略時はすべてのPRIインターフェースの情報が表示される。

COUNTER: 表示するカウンターの種類を指定する。カウンターには、DIAGNOSTIC（診断カウンター）、INTERFACE（インターフェースMIB）、LINK（過去24時間の統計情報）、PRI（プライベートMIB）がある。種類を指定しなかったときはLINKを除くすべてのカテゴリーが表示される。

CHANNEL: チャンネル番号。表示する情報を指定したチャンネルだけに制限する。COUNTERパラメーターにINTERFACEを指定したときは無効。

HISTORY: LINKカウンター（COUNTER=LINK）において、過去24時間中の特定の期間の情報だけを表示させたいときに指定する。

NEAR: LINKカウンター（COUNTER=LINK）において、リンクのローカル側の情報だけを表示する。

FAR: LINKカウンター（COUNTER=LINK）において、リンクのリモート側の情報だけを表示する。

BOTH: LINKカウンター（COUNTER=LINK）において、リンク両端の情報を表示する。これがデフォルト。

入力・出力・画面例

    Manager > show pri counter

    PRI instance 0:        784 seconds      Last change at:          0 seconds

    Interface MIB Counters

        Receive:                               Transmit:
    ifInOctets                       0     ifOutOctets                   2739
    ifInUcastPkts                    0     ifOutUcastPkts                 227
    ifInNUcastPkts                   0     ifOutNUcastPkts                  0
    ifInDiscards                     0     ifOutDiscards                    0
    ifInErrors                       0     ifOutErrors                      0
    ifInUnknownProtos                0     ifOutQLen                        0

    Interface-global Diagnostic Counters

      Device Independent Diagnostic Counters

    EventQueueFulls                  0

    Near End Event Counters (current interval)
      PathFailures                   0     SeverelyErroredFrames            0
      LineCodeViolations             0     ControlledSlips                  0
      PathCodingViolations           0

    Near End Time Counters (current interval)
      TotalSecs                    136     PercentageErrorFreeSecs      0.00%
      UnavailableSecs              136     SeverelyErroredSecs              0
      SeverelyErroredFSecs           0     SeverelyErroredLSecs             0
      ErroredSecs                    0     LineErroredSecs                  0
      SingleErroredSecs              0     BurstyErroredSecs                0
      LossOfSignalSecs               0     AISSecs                          0
      ControlledSlipSecs             0     DegradedMins                     0

    Near End Event Counters (last 24 hours)
      PathFailures                   0     SeverelyErroredFrames            0
      LineCodeViolations             0     ControlledSlips                  0
      PathCodingViolations           0

    Near End Time Counters (last 24 hours)
      TotalSecs                    639     PercentageErrorFreeSecs      0.00%
      UnavailableSecs              639     SeverelyErroredSecs              0
      SeverelyErroredFSecs           0     SeverelyErroredLSecs             0
      ErroredSecs                    0     LineErroredSecs                  0
      SingleErroredSecs              0     BurstyErroredSecs                0
      LossOfSignalSecs               0     AISSecs                          0
      ControlledSlipSecs             0     DegradedMins                     0

    Far End Event Counters (current interval)
      PathFailures                   0     PathCodingViolations             0

    Far End Time Counters (current interval)
      TotalSecs                    136     PercentageErrorFreeSecs    100.00%
      UnavailableSecs                0     SeverelyErroredSecs              0
      SeverelyErroredFSecs           0
      ErroredSecs                    0     LineErroredSecs                  0
      SingleErroredSecs              0     BurstyErroredSecs                0
      ControlledSlipSecs             0     DegradedMins                     0

    Far End Event Counters (last 24 hours)
      PathFailures                   0     PathCodingViolations             0

    Far End Time Counters (last 24 hours)
      TotalSecs                    639     PercentageErrorFreeSecs    100.00%
      UnavailableSecs                0     SeverelyErroredSecs              0
      SeverelyErroredFSecs           0
      ErroredSecs                    0     LineErroredSecs                  0
      SingleErroredSecs              0     BurstyErroredSecs                0
      ControlledSlipSecs             0     DegradedMins                     0

    Channel Counters

    Channel 1:   Slots: 1-8

      PRI Counters

        Receive:                               Transmit:
    Frames                           0     Frames                          51
    OverlengthFrames                 0     CTSLosts                         0
    UnderlengthFrames                0     Underruns                        0
    CRCErrors                        0     LostInterrupts                   0
    Aborts                           0     DroppedFrames                    0
    NonOctetAligneds                 0     NoPackets                        0
    Overruns                         0
    NonmatchAddresses                0     QueueLength                      0
    Misseds                          0     Recovers                         0
    TooFewBuffers                    0     SDMABusErrors                    0
    QueueLength                      0     CommandTimeouts                  0
                                           LastCommand                      0

      No Device Dependent Diagnostic Counters for this channel

    D Channel:   Slot: Slots: - (channel inactive)

      PRI Counters

        Receive:                               Transmit:
    Frames                           0     Frames                         176
    OverlengthFrames                 0     CTSLosts                         0
    UnderlengthFrames                0     Underruns                        0
    CRCErrors                        0     LostInterrupts                   0
    Aborts                           0     DroppedFrames                    0
    NonOctetAligneds                 0     NoPackets                        0
    Overruns                         0     HighPriorityFrames               0
    NonmatchAddresses                0     QueueLength                      0
    Misseds                          0     Recovers                         1
    TooFewBuffers                    0     SDMABusErrors                    0
    QueueLength                      0     CommandTimeouts                  0
                                           LastCommand                      0

      No Device Dependent Diagnostic Counters for this channel

関連コマンド

RESET PRI COUNTER
SHOW PRI CONFIGURATION

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H