[index] CentreCOM AR550S コマンドリファレンス 2.9

# SET PPP ACSERVICE

カテゴリー：PPP / PPPoE AC

`SET PPP ACSERVICE=service-name [ACRADIUS={OFF|ON}] [MAXSESSIONS=1..512] [TEMPLATE=template]`

service-name: PPPoEサービス名（最大64文字）
template: PPPテンプレート番号（0〜31）

PPPoEサービスの設定を変更する。

パラメーター

ACSERVICE: サービス名。クライアント側でこの名前を指定して接続する。

TEMPLATE: PPPテンプレート番号。クライアントが接続してきたときに動的に作成するPPPインターフェースのパラメーターをあらかじめ設定したもの。CREATE PPP TEMPLATEコマンドで作成する。

ACRADIUS: RADIUS認証を行うかどうか。ONの場合、PPPoEクライアントのMACアドレスを元にRADIUSサーバーに問い合わせる。ただし、前提として、PPPテンプレートでLOGIN=RADIUSを指定しておく必要がある。

MAXSESSIONS: PPPoE同時最大セッション数。デフォルトは1。

関連コマンド

ADD PPP ACSERVICE
CREATE PPP
CREATE PPP TEMPLATE
DESTROY PPP
DESTROY PPP TEMPLATE
DISABLE PPP ACCESSCONCENTRATOR
ENABLE PPP ACCESSCONCENTRATOR

参考

RFC1331, The Point-to-Point Protocol (PPP) for the Transmission of Multi-protocol Datagrams over Point-to-Point Links
RFC1332, The PPP Internet Protocol Control Protocol (IPCP)
RFC1333, PPP Link Quality Monitoring
RFC1334, PPP Authentication Protocols
RFC1378, The PPP AppleTalk Control Protocol (ATCP)
RFC1548, The Point-to-Point Protocol (PPP)
RFC1549, PPP in HDLC Framing
RFC1552, The PPP Internetwork Packet Exchange Control Protocol (IPXCP)
RFC1570, PPP LCP Extensions
RFC1638, PPP Bridging Control Protocol (BCP)
RFC1661, The Point-to-Point Protocol (PPP)
RFC1662, PPP in HDLC-like Framing
RFC1877, PPP Internet Protocol Control Protocol Extensions for Name Server Addresses
RFC1962, The PPP Compression Control Protocol (CCP)
RFC1968, The PPP Encryption Control Protocol (ECP)
RFC1974, PPP Stac LZS Compression Protocol
RFC1978, PPP Predictor Compression Protocol
RFC1990, The PPP Multilink Protocol (MP)
RFC2125, The PPP Bandwidth Allocation Protocol (BAP) / The PPP Bandwidth Allocation Control Protocol (BACP)
RFC2516, A Method for Transmitting PPP Over Ethernet (PPPoE)

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H