## CentreCOM AR550S 設定例集 2.9
##  120 トンネリングによるIPv6インターネット接続（専用線環境）
##  ルーターのコンフィグ

SET BRI=0 MODE=TDM ACTIVATION=ALWAYS TDMSLOTS=1-2
CREATE TDM GROUP=ISP INT=bri0 SLOTS=1-2
CREATE PPP=0 OVER=TDM-ISP LQR=OFF
ENABLE IP
ADD IP INT=eth0 IP=4.4.4.1 MASK=255.255.255.248
ADD IP INT=vlan1 IP=192.168.10.1 MASK=255.255.255.0
ADD IP INT=ppp0 IP=0.0.0.0
ADD IP ROUTE=0.0.0.0 INT=ppp0 NEXTHOP=0.0.0.0
ENABLE FIREWALL
CREATE FIREWALL POLICY=net
ENABLE FIREWALL POLICY=net LOG=DENY
ENABLE FIREWALL POLICY=net ICMP_F=PING,UNREACHABLE
DISABLE FIREWALL POLICY=net IDENTPROXY
ADD FIREWALL POLICY=net INT=eth0 TYPE=PRIVATE
ADD FIREWALL POLICY=net INT=vlan1 TYPE=PRIVATE
ADD FIREWALL POLICY=net INT=ppp0 TYPE=PUBLIC
ADD FIREWALL POLICY=net NAT=ENHANCED INT=vlan1 GBLINT=ppp0 GBLIP=4.4.4.1
ADD FIREWALL POLICY=net RULE=1 AC=ALLOW INT=ppp0 PROTO=TCP IP=4.4.4.2 PORT=80
ADD FIREWALL POLICY=net RULE=2 AC=ALLOW INT=ppp0 PROTO=TCP IP=4.4.4.3 PORT=25
ADD FIREWALL POLICY=net RULE=3 AC=ALLOW INT=ppp0 PROTO=TCP IP=4.4.4.4 PORT=53
ADD FIREWALL POLICY=net RULE=4 AC=ALLOW INT=ppp0 PROTO=UDP IP=4.4.4.4 PORT=53
ADD FIREWALL POLICY=net RULE=5 AC=ALLOW INT=ppp0 PROTO=41 IP=4.4.4.1 GBLIP=4.4.4.1 REMOTEIP=1.2.3.4
ENABLE IPV6
ADD IPV6 INT=eth0 IP=3ffe:1:1:1::1/64 PUBLISH=YES
ADD IPV6 INT=vlan1 IP=3ffe:1:1:2::1/64 PUBLISH=YES
ENABLE IPV6 ADVERTISE
ADD IPV6 TUNNEL LOCAL=4.4.4.1 TARGET=1.2.3.4
ADD IPV6 ROUTE=::/0 INT=virt0 NEXT=::
ADD IPV6 FILTER=1 SOURCE=:: ACTION=INCLUDE
SET IPV6 FILTER=1 ENTRY=1 DEST=3ffe:1:1::/48 PROTO=TCP SESS=ESTABLISHED
ADD IPV6 FILTER=1 SOURCE=:: ACTION=INCLUDE
SET IPV6 FILTER=1 ENTRY=2 DEST=3ffe:1:1::/48 PROTO=UDP SPORT=53
ADD IPV6 FILTER=1 SOURCE=:: ACTION=INCLUDE
SET IPV6 FILTER=1 ENTRY=3 DEST=3ffe:1:1:1::2/128 PROTO=TCP DPORT=80
ADD IPV6 FILTER=1 SOURCE=:: ACTION=INCLUDE
SET IPV6 FILTER=1 ENTRY=4 DEST=3ffe:1:1:1::3/128 PROTO=TCP DPORT=25
ADD IPV6 FILTER=1 SOURCE=:: ACTION=INCLUDE
SET IPV6 FILTER=1 ENTRY=5 DEST=3ffe:1:1:1::4/128 PROTO=UDP DPORT=53
ADD IPV6 FILTER=1 SOURCE=:: ACTION=INCLUDE
SET IPV6 FILTER=1 ENTRY=6 DEST=3ffe:1:1:1::4/128 PROTO=TCP DPORT=53
ADD IPV6 FILTER=1 SOURCE=:: ACTION=INCLUDE
SET IPV6 FILTER=1 ENTRY=7 DEST=:: PROTO=ICMP ICMPTYPE=ANY ICMPCODE=ANY
SET IPV6 INT=virt0 FILTER=1
