## CentreCOM AR550S 設定例集 2.9
##  163 CUGサービスを利用した拠点間のPIM-DMによるIPマルチキャストルーティング（L2TP＋IPsec）
##  ルーターBのコンフィグ
##
## 「#」で始まる行は、コンソールから入力しないと意味を持たないコマンドです。

ADD USER=secoff PASSWORD=PasswordS PRIVILEGE=SECURITYOFFICER
ENABLE L2TP
ENABLE L2TP SERVER=BOTH
ADD L2TP PASSWORD=l2tpB
ADD L2TP CALL=remote1 REMOTE=remote1 TYPE=VIRTUAL IP=172.16.0.1 PRECEDENCE=IN PASSWORD=l2tpA 
CREATE PPP=0 OVER=eth0-ANY
SET PPP=0 OVER=eth0-ANY BAP=OFF IPREQUEST=ON USER=userB@cug PASSWORD=cugpasswdB LQR=OFF ECHO=ON
CREATE PPP=11 OVER=TNL-remote1 IDLE=ON BAP=OFF LQR=OFF
ENABLE IP
ENABLE IP REMOTEASSIGN
ADD IP INT=vlan1 IP=192.168.20.1 MASK=255.255.255.0
ADD IP INT=ppp0 IP=0.0.0.0
ADD IP INT=ppp11 IP=172.16.1.2 MASK=255.255.255.0
ADD IP ROUTE=172.16.0.1 MASK=255.255.255.255 INTERFACE=ppp0 NEXTHOP=0.0.0.0
ADD IP RIP INT=ppp11 SEND=RIP2 RECEIVE=RIP2
ENABLE IP IGMP
ENABLE IP IGMP INT=ppp11
ENABLE IP IGMP INT=vlan1
ENABLE PIM
ADD PIM INT=ppp11 MODE=DENSE
ADD PIM INT=vlan1 MODE=DENSE
ENABLE FIREWALL
CREATE FIREWALL POLICY=net
ENABLE FIREWALL POLICY=net ICMP_F=PING,UNREACH
DISABLE FIREWALL POLICY=net IDENTPROXY
ADD FIREWALL POLICY=net INT=vlan1 TYPE=PRIVATE
ADD FIREWALL POLICY=net INT=ppp11 TYPE=PRIVATE
ADD FIREWALL POLICY=net INT=ppp0 TYPE=PUBLIC
ADD FIREWALL POLICY=net RULE=1 AC=ALLOW INT=ppp0 PROT=UDP PO=500 IP=172.16.0.2 
ADD FIREWALL POLICY=net RULE=2 AC=ALLOW INT=ppp0 PROT=UDP PO=1701 IP=172.16.0.2
# CREATE ENCO KEY=1 TYPE=GENERAL VALUE="secret1"
# LOGIN secoff
# ENABLE SYSTEM SECURITY_MODE
CREATE ISAKMP POLICY="i-1" PEER=172.16.0.1 KEY=1 SENDN=TRUE HEARTBEATMODE=BOTH
CREATE IPSEC SASPEC=1 KEYMAN=ISAKMP PROTOCOL=ESP ENCALG=DES HASHALG=SHA
CREATE IPSEC BUNDLE=1 KEYMAN=ISAKMP STRING="1"
CREATE IPSEC POLICY="isa" INT=ppp0 ACTION=PERMIT LPORT=500 RPORT=500 TRANSPORT=UDP
CREATE IPSEC POLICY="vpn-1" INTERFACE=ppp0 ACTION=IPSEC KEYMAN=ISAKMP BUNDLE=1 PEER=172.16.0.1
SET IPSEC POLICY="vpn-1" LAD=172.16.0.2 LPORT=1701 RAD=172.16.0.1 RPORT=1701
ENABLE IPSEC
ENABLE ISAKMP
