[index] CentreCOM AR550S コマンドリファレンス 2.9

# SET IPSEC BUNDLESPECIFICATION

カテゴリー：IPsec / SAバンドルスペック

`SET IPSEC BUNDLESPECIFICATION=bspec-id [EXPIRYKBYTES=1..4193280] [EXPIRYSECONDS=300..31449600]`

bspec-id: SAバンドルスペック番号（0〜255）

SAバンドルスペックの設定パラメーターを変更する。

パラメーター

BUNDLESPECIFICATION: SAバンドルスペック番号

EXPIRYKBYTES: バンドル内SAの有効期限（Kbyte）。通信データ量がここで指定した量に達すると、該当SAバンドルは再ネゴシエートされる。KEYMANAGEMENTパラメーターにISAKMPを指定したときだけ有効。4193280を超える値を指定した場合、4193280が設定される。デフォルトは無期限。

EXPIRYSECONDS: バンドル内SAの有効期限（秒）。バンドル作成後ここで指定した時間が経過すると、該当SAバンドルは再ネゴシエートされる。KEYMANAGEMENTパラメーターにISAKMPを指定したときだけ有効。デフォルトは28800秒（8時間）。

関連コマンド

CREATE IPSEC BUNDLESPECIFICATION
DESTROY IPSEC BUNDLESPECIFICATION
SHOW IPSEC BUNDLESPECIFICATION

参考

RFC2401, Security Architecture for the Internet Protocol
RFC2402, IP Authentication Header
RFC2403, The Use of HMAC-MD5-96 within ESP and AH
RFC2404, The Use of HMAC-SHA-1-96 within ESP and AH
RFC2405, The ESP DES-CBC Cipher Algorithm With Explicit IV
RFC2406, IP Encapsulating Security Payload (ESP)
RFC2407, The Internet IP Security Domain of Interpretation for ISAKMP
RFC2408, Internet Security Association and Key Management Protocol (ISAKMP)
RFC2409, The Internet Key Exchange (IKE)
RFC2410, The NULL Encryption Algorithm and Its Use With IPsec
RFC2411, IP Security Document Roadmap
RFC2412, The OAKLEY Key Determination Protocol
RFC2451, The ESP CBC-Mode Cipher Algorithms
RFC2104, HMAC: Keyed-Hashing for Message Authentication

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H