[index] CentreCOM AR550S コマンドリファレンス 2.9

# RESET ISAKMP COUNTER

カテゴリー：IPsec / ISAKMP

`RESET ISAKMP COUNTER[={GENERAL|MAIN|QUICK|SAD|SPD|XDB|IPSEC|INFO|AGGRESSIVE|NETWORK|TRANSACTION}]`

ISAKMPモジュールの統計カウンターをクリアする。

パラメーター

COUNTER: クリアするカウンターのカテゴリーを指定する。省略時はすべてのカウンターがクリアされる。カテゴリーには、GENERAL（一般情報）、MAIN（Mainモード交換）、QUICK（Quickモード交換）、SAD（ISAKMP SAデータベース）、SPD（ISAKMPセキュリティーポリシーデータベース）、XDB（ISAKMP交換データベース）、IPSEC（ISAKMPとIPsecのインターフェースカウンター）、INFO（Informational交換）、AGGRESSIVE（Aggressiveモード交換）、NETWORK（ISAKMPメッセージの送受信）、TRANSACTION（Transaction交換）がある。

関連コマンド

SHOW ISAKMP COUNTERS

参考

RFC2401, Security Architecture for the Internet Protocol
RFC2402, IP Authentication Header
RFC2403, The Use of HMAC-MD5-96 within ESP and AH
RFC2404, The Use of HMAC-SHA-1-96 within ESP and AH
RFC2405, The ESP DES-CBC Cipher Algorithm With Explicit IV
RFC2406, IP Encapsulating Security Payload (ESP)
RFC2407, The Internet IP Security Domain of Interpretation for ISAKMP
RFC2408, Internet Security Association and Key Management Protocol (ISAKMP)
RFC2409, The Internet Key Exchange (IKE)
RFC2410, The NULL Encryption Algorithm and Its Use With IPsec
RFC2411, IP Security Document Roadmap
RFC2412, The OAKLEY Key Determination Protocol
RFC2451, The ESP CBC-Mode Cipher Algorithms
RFC2104, HMAC: Keyed-Hashing for Message Authentication

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H