[index] CentreCOM AR550S コマンドリファレンス 2.9

# SET SNMP COMMUNITY

カテゴリー：運用・管理 / SNMP

`SET SNMP COMMUNITY=community [ACCESS={READ|WRITE}] [OPEN={ON|OFF|YES|NO|TRUE|FALSE}]`

community: SNMPコミュニティー名（1〜15文字。大文字小文字を区別する）

（SNMPv1/v2c）SNMPコミュニティーの設定パラメーターを変更する。

パラメーター

COMMUNITY: SNMPコミュニティー名

ACCESS: コミュニティーのアクセス権を指定する。READ（デフォルト）は読み出し（get、get-next）のみを許可、WRITEは読み書き両方（get、get-next、set）を許可する。

OPEN: SNMPオペレーションをすべてのホストに開放するかどうかを示す。NO（デフォルト）は、MANAGERパラメーターで指定したホストのみに制限することを示す。YESを指定すると、すべてのSNMP要求を受け入れる。ON、YES、TRUEおよびOFF、NO、FALSEはそれぞれ同じ意味。

関連コマンド

CREATE SNMP COMMUNITY
DESTROY SNMP COMMUNITY
SHOW SNMP COMMUNITY

参考

RFC1157, A Simple Network Management Protocol (SNMP)
RFC1213, Management Information Base for Network Management of TCP/IP-based internets: MIB-II
RFC1901, Introduction to Community-based SNMPv2
RFC1902, Structure of Management Information for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1903, Textual Conventions for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1904, Conformance Statements for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1905, Protocol Operations for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1906, Transport Mappings for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1907, Management Information Base for Version 2 of the Simple Network Management Protocol (SNMPv2)

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H