[index] CentreCOM AR550S コマンドリファレンス 2.9

# DISABLE BGP DAMPING

カテゴリー：IP / 経路制御（BGP-4）

`DISABLE BGP DAMPING [PARAMETERSET={ALL|0..100}]`

BGP-4ルートフラップダンピングを無効にする。デフォルトは無効。
本コマンドでは、特定のパラメーターセットだけを無効化することもできる。この場合でも、すべてのパラメーターセットを無効化すると、ルートフラップダンピング機能全体も自動的に無効化される。

パラメーター

PARAMETERSET: パラメーターセット番号。パラメーターセット番号を指定した場合は、該当パラメーターセットだけが対象となる。0はデフォルトのパラメーターセット。ALLを指定した場合、および、番号を省略した場合は、すべてのパラメーターセットが対象となる。

関連コマンド

ADD BGP PEER
CREATE BGP DAMPING PARAMETERSET
DESTROY BGP DAMPING PARAMETERSET
ENABLE BGP DAMPING
PURGE BGP DAMPING
RESET BGP DAMPING
SET BGP DAMPING PARAMETERSET
SHOW BGP DAMPING
SHOW BGP DAMPING ROUTES

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2439, BGP Route Flap Damping
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H