## CentreCOM AR550S 設定例集 2.9
##  48 PPPoEによる端末型インターネット接続（スタティックENAT）
##  ルーターのコンフィグ

CREATE PPP=0 OVER=eth0-ANY
SET PPP=0 OVER=eth0-ANY USER=user@isp PASSWORD=isppasswd LQR=OFF BAP=OFF ECHO=ON
ENABLE IP
ADD IP INT=vlan1 IP=192.168.10.1 MASK=255.255.255.0
ADD IP INT=ppp0 IP=12.34.56.78 MASK=255.255.255.255
ADD IP ROUTE=0.0.0.0 INT=ppp0 NEXTHOP=0.0.0.0
ADD IP DNS PRIMARY=12.34.11.11 SECONDARY=12.34.11.22
ENABLE IP DNSRELAY
ENABLE FIREWALL
CREATE FIREWALL POLICY=net
ENABLE FIREWALL POLICY=net ICMP_F=PING,UNREACH
DISABLE FIREWALL POLICY=net IDENTPROXY
ADD FIREWALL POLICY=net INT=vlan1 TYPE=PRIVATE
ADD FIREWALL POLICY=net INT=ppp0 TYPE=PUBLIC
ADD FIREWALL POLICY=net NAT=ENHANCED INT=vlan1 GBLINT=ppp0
ADD FIREWALL POLICY=net RULE=1 AC=ALLOW INT=ppp0 PROTO=TCP GBLIP=12.34.56.78 GBLPORT=80 IP=192.168.10.5 PORT=80
ENABLE DHCP
CREATE DHCP POLICY=BASE LEASETIME=7200
ADD DHCP POLICY=BASE SUBNET=255.255.255.0 ROUTER=192.168.10.1 DNSSERVER=192.168.10.1
CREATE DHCP RANGE=LOCAL POLICY=BASE IP=192.168.10.100 NUMBER=32 PROBE=ARP
