## CentreCOM AR550S 設定例集 2.9
##  131 PPPoEインターネット接続環境における3点間IPsec VPN（支社間通信は本社経由、全拠点アドレス固定）
##  ルーターBのコンフィグ
##
## 「#」で始まる行は、コンソールから入力しないと意味を持たないコマンドです。

ADD USER=secoff PASSWORD=PasswordS PRIVILEGE=SECURITYOFFICER
CREATE PPP=0 OVER=eth0-ANY
SET PPP=0 OVER=eth0-ANY USER=user@ispB PASSWORD=isppasswdB LQR=OFF BAP=OFF ECHO=ON
ENABLE IP
ADD IP INT=vlan1 IP=192.168.20.1 MASK=255.255.255.0
ADD IP INT=ppp0 IP=200.100.20.1 MASK=255.255.255.255
ADD IP ROUTE=0.0.0.0 INT=ppp0 NEXTHOP=0.0.0.0
ENABLE FIREWALL
CREATE FIREWALL POLICY=net
ENABLE FIREWALL POLICY=net ICMP_F=PING,UNREACHABLE
DISABLE FIREWALL POLICY=net IDENTPROXY
ADD FIREWALL POLICY=net INT=vlan1 TYPE=PRIVATE
ADD FIREWALL POLICY=net INT=ppp0 TYPE=PUBLIC
ADD FIREWALL POLICY=net NAT=ENHANCED INT=vlan1 GBLINT=ppp0
ADD FIREWALL POLICY=net RULE=1 AC=ALLOW INT=ppp0 PROT=UDP PORT=500 IP=200.100.20.1 GBLIP=200.100.20.1 GBLPORT=500
ADD FIREWALL POLICY=net RULE=2 AC=NONAT INT=vlan1 PROT=ALL IP=192.168.20.1-192.168.20.254
SET FIREWALL POLICY=net RULE=2 REMOTEIP=192.168.0.1-192.168.255.254
ADD FIREWALL POLICY=net RULE=3 AC=NONAT INT=ppp0 PROT=ALL IP=192.168.20.1-192.168.20.254 ENCAP=IPSEC
# CREATE ENCO KEY=1 TYPE=GENERAL VALUE="secret-ab"
CREATE ISAKMP POLICY="i_A" PEER=200.100.10.1 KEY=1 SENDN=TRUE HEARTBEATMODE=BOTH
CREATE IPSEC SASPEC=1 KEYMAN=ISAKMP PROTOCOL=ESP ENCALG=DES HASHALG=SHA
CREATE IPSEC BUNDLE=1 KEYMAN=ISAKMP STRING="1"
CREATE IPSEC POLICY="isa" INT=ppp0 ACTION=PERMIT LPORT=500 RPORT=500 TRANSPORT=UDP
CREATE IPSEC POLICY="vpn_A" INT=ppp0 ACTION=IPSEC KEYMAN=ISAKMP BUNDLE=1 PEER=200.100.10.1
SET IPSEC POLICY="vpn_A" LAD=192.168.20.0 LMA=255.255.255.0 RAD=192.168.0.0 RMA=255.255.0.0
CREATE IPSEC POLICY="inet" INT=ppp0 ACTION=PERMIT
ENABLE IPSEC
ENABLE ISAKMP
# LOGIN secoff
# ENABLE SYSTEM SECURITY_MODE
