IPv6マルチキャスト

サブカテゴリー別索引

設定例

[A] [D] [E] [P] [R] [S]

    A (top)

    ADD PIM6 BSRCANDIDATE
    ADD PIM6 INTERFACE
    ADD PIM6 RPCANDIDATE

    D (top)

    DELETE PIM6 BSRCANDIDATE
    DELETE PIM6 INTERFACE
    DELETE PIM6 RPCANDIDATE
    DISABLE IPV6 MLD
    DISABLE IPV6 MLD DEBUG
    DISABLE IPV6 MLD INTERFACE
    DISABLE IPV6 MLD PROXY
    DISABLE PIM6

    E (top)

    ENABLE IPV6 MLD
    ENABLE IPV6 MLD DEBUG
    ENABLE IPV6 MLD INTERFACE
    ENABLE IPV6 MLD PROXY
    ENABLE PIM6

    P (top)

    PURGE PIM6

    R (top)

    RESET PIM6 INTERFACE

    S (top)

    SET IPV6 MLD
    SET IPV6 MLD INTERFACE
    SET PIM6
    SET PIM6 BSRCANDIDATE
    SET PIM6 INTERFACE
    SET PIM6 RPCANDIDATE
    SHOW IPV6 MLD
    SHOW IPV6 MLD CONFIG
    SHOW IPV6 MLD COUNTERS
    SHOW IPV6 MLD DEBUG
    SHOW IPV6 MLD PROXY
    SHOW IPV6 MLD PROXY INTERFACE
    SHOW IPV6 ROUTE MULTICAST
    SHOW PIM6