[index] CentreCOM AR550S コマンドリファレンス 2.9

# SHOW PPP IDLETIMER

カテゴリー：PPP / PPPインターフェース

`SHOW PPP[=ppp-interface] IDLETIMER`

ppp-interface: PPPインターフェース番号（0〜511）

PPPインターフェースの無通信時切断タイマー（アイドルタイマー）の情報を表示する。

パラメーター

PPP: PPPインターフェース番号

入力・出力・画面例

    Manager bulbul> show ppp idletimer

      Interface
        Configured Idle Time       Idle Timer Value
      ---------------------------------------------
      ppp0
                         OFF                    OFF
      ---------------------------------------------

      Interface
        Configured Idle Time       Idle Timer Value
      ---------------------------------------------
      ppp1
                         300                    285
      ---------------------------------------------

表 1
Interface | インターフェース名
Configured Idle Time | アイドルタイマーの設定値（秒）
Idle Timer Value | アイドルタイマーの残り時間。EXPIREDはタイマーがゼロになったことを示す

関連コマンド

SHOW PPP
SHOW PPP CONFIG
SHOW PPP COUNTER
SHOW PPP MULTILINK

参考

RFC1331, The Point-to-Point Protocol (PPP) for the Transmission of Multi-protocol Datagrams over Point-to-Point Links
RFC1332, The PPP Internet Protocol Control Protocol (IPCP)
RFC1333, PPP Link Quality Monitoring
RFC1334, PPP Authentication Protocols
RFC1548, The Point-to-Point Protocol (PPP)
RFC1549, PPP in HDLC Framing
RFC1570, PPP LCP Extensions
RFC1638, PPP Bridging Control Protocol (BCP)
RFC1661, The Point-to-Point Protocol (PPP)
RFC1662, PPP in HDLC-like Framing
RFC1877, PPP Internet Protocol Control Protocol Extensions for Name Server Addresses
RFC1990, The PPP Multilink Protocol (MP)
RFC2125, The PPP Bandwidth Allocation Protocol (BAP) / The PPP Bandwidth Allocation Control Protocol (BACP)
RFC2516, A Method for Transmitting PPP Over Ethernet (PPPoE)

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H