[index] CentreCOM AR550S コマンドリファレンス 2.9

# SET IPSEC UDPPORT

カテゴリー：IPsec / 一般コマンド

`SET IPSEC UDPPORT=port`

port: UDPポート番号（0〜65535）

UDPトンネリング（ESP over UDP）パケットを送受信するUDPポートを変更する。デフォルトは2746番。

パラメーター

UDPPORT: UDPポート番号。デフォルトは2746

関連コマンド

SHOW IPSEC

参考

RFC2401, Security Architecture for the Internet Protocol
RFC2402, IP Authentication Header
RFC2403, The Use of HMAC-MD5-96 within ESP and AH
RFC2404, The Use of HMAC-SHA-1-96 within ESP and AH
RFC2405, The ESP DES-CBC Cipher Algorithm With Explicit IV
RFC2406, IP Encapsulating Security Payload (ESP)
RFC2407, The Internet IP Security Domain of Interpretation for ISAKMP
RFC2408, Internet Security Association and Key Management Protocol (ISAKMP)
RFC2409, The Internet Key Exchange (IKE)
RFC2410, The NULL Encryption Algorithm and Its Use With IPsec
RFC2411, IP Security Document Roadmap
RFC2412, The OAKLEY Key Determination Protocol
RFC2451, The ESP CBC-Mode Cipher Algorithms
RFC2104, HMAC: Keyed-Hashing for Message Authentication

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H