[index] CentreCOM AR550S コマンドリファレンス 2.9

# SHOW ENCO COUNTERS

カテゴリー：暗号・圧縮 / 一般コマンド

`SHOW ENCO COUNTERS={AES|DES|DH|HARDWARE|HMAC|JOBPROCESSING|RSA|USER|UTIL}`

暗号（ENCO）モジュールの各種統計カウンターを表示する。

パラメーター

COUNTERS: 表示する統計カウンターを指定する。USER（ENCOモジュールを利用する上位モジュール）、UTIL（ユーティリティージョブ）、HARDWARE（暗号処理ハードウェア）、JOBPROCESSINGは、ENCOモジュールの全般的情報を示すもの。AES、DES、DH（Diffie Hellman）、HMAC、RSAは個々の暗号プロセスを対象としたもの。

入力・出力・画面例

    SecOff > show enco counters=des

    ENCO Process DES/3DES Counters:
      configGood ...................... 6       configBad ....................... 0
      configNoResource ................ 0       configNotSSH .................... 0
      badBuffer ....................... 0       badAlign ........................ 0
      badLength ....................... 0       nohistory ....................... 0
      desJobs ...................... 2710       3Des2KeyJobs .................... 0
      3DesInnerJobs ................... 0       d3DesOuterJobs .................. 0
      noHistJobs ................... 2710       desMacJobs ...................... 0
      badDesType ...................... 0       badJobType ...................... 0

      unknownJob ...................... 0       error ........................... 0
      reset ........................... 0       confNotDes ...................... 0
      commWaitTimeOut ................. 0       dataInnWaitTimeOut .............. 0
      dataOutWaitTimeOut .............. 0

      goodDecrypt .................. 1368       goodEncrypt .................. 1342
      badDecrypt ...................... 0       badEncrypt ...................... 0

    SecOff > show enco counters=dh

    ENCO Process Diffie Hellman Counters:
      goodPhase1 ...................... 1       badPhase1 ....................... 0
      goodPhase2 ...................... 1       badPhase2 ....................... 0
      badGroupType .................... 0       badGroup ........................ 0
      badGroupParameters .............. 0       badDataLength ................... 0
      noResources ..................... 0

    SecOff > show enco counters=hmac

    ENCO Process HMAC Counters:
      goodHashMD5 .................. 2877       badHashMD5 ...................... 0
      goodHashSHA .................. 2877       badHashSHA ...................... 0
      goodConfigure ................... 0       badConfigure .................... 0
      badAlgorithm .................... 0       noResources ..................... 0
      badKeyLength .................... 0       unknownJob ...................... 0
      badDataLength ................... 0

    SecOff > show enco counters=jobprocessing

      ENCO Queues                          Queued  Discarded  Processed
      -----------------------------------------------------------------
         Immediate Input queue                  0          0          0
         Priority 0 Input queue (high)          0          0          0
         Priority 1 Input queue                 0          0          0
         Priority 2 Input queue                 0          0          0
         Priority 3 Input queue                 0          0          0
         Priority 4 Input queue                 0          0          9
         Priority 5 Input queue                 0          0       8715
         Priority 6 Input queue                 0          0          0
         Priority 7 Input queue                 0          0          0
         Priority 8 Input queue (low)           0          0          0
         Output queue                           0          0       8724
      -----------------------------------------------------------------

      Input queue length limit ......... 250
      Lowest input priority queue ...... 5
      Highest input priority queue ..... 0

    SecOff > show enco counters=rsa

    ENCO Process RSA Counters:
      goodPublicEncrypt ............... 0       badPublicEncrypt ................ 0
      goodPrivateDecrypt .............. 0       badPrivateDecrypt ............... 0
      goodPrivateEncrypt .............. 0       badPrivateEncrypt ............... 0
      goodPublicDecrypt ............... 0       badPublicDecrypt ................ 0
      goodGenerateKey ................. 2       badGenerateKey .................. 0
      badDataLength ................... 0       badKey .......................... 0

    SecOff > show enco counters=user

    ENCO User Interface Counters:
      startConfig ..................... 3       startReconfig ................... 0
      attachGood ...................... 3       attachFail ...................... 0
      attachNoConfig .................. 0       attachBadUserType ............... 0
      attachedInvalidChan ............. 0       attachedUnusedChan .............. 0
      attachProcNotAvail .............. 0

      reconfigInvalidChan ............. 0       reconfigUnusedChan .............. 0
      reconfigNoConfig ................ 0

      detachInvalidChannel ............ 0       detachUnusedChannel ............. 0
      detachedInvalidChan ............. 0       detachedUnusedChan .............. 0
      detachGood ...................... 0

      decodeInvalidChannel ............ 0       decodeUnusedChannel ............. 0
      encodeInvalidChannel ............ 0       encodeUnusedChannel ............. 0
      codedInvalidChannel ............. 0       codedUnusedChannel .............. 0
      resetInvalidChannel ............. 0       resetUnusedChannel .............. 0
      resetDoneInvalidChan ............ 0       resetDoneUnusedChan ............. 0

      configBadMode ................... 0       configBadUserType ............... 0
      configBadPktLength .............. 0       configBadEncrType ............... 0
      configBadCompType ............... 0       configBadHistoryMode ............ 0
      configBadCheckType .............. 0

      discardInvalidChan .............. 0       discardUnusedChannel ............ 0

    SecOff > show enco counters=util

    ENCO Utility Counters:
      codeNullPacket .................. 0       codeBadPacketPriorit ............ 0
      codeBadPacketLength ............. 0       codeBadConfig ................... 0
      actionSentEncode ................ 0       actionSentDecode ................ 0
      configureGood ................... 9       configureFail ................... 0
      encodeGood ...................... 6       decodeGood ...................... 3
      encodeBad ....................... 0       decodeBad ....................... 0

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H