[index] CentreCOM AR550S コマンドリファレンス 2.9

# SHOW IPSEC

カテゴリー：IPsec / 一般コマンド

`SHOW IPSEC`

IPsecモジュールの状態を表示する。

入力・出力・画面例

    SecOff > show ipsec

    IPSEC Module Configuration

      Module Status .......................... ENABLED
      IPsec over UDP
        Status ............................... CLOSED
        Listen Port .......................... 2746

表 1
Module Status | IPsecモジュールの有効・無効
IPsec over UDP/Status | UDPトンネリング（ESP over UDP）の有効・無効
IPsec over UDP/Listen Port | UDPトンネリングパケットの送受信ポート番号

関連コマンド

DISABLE IPSEC
ENABLE IPSEC

参考

RFC2401, Security Architecture for the Internet Protocol
RFC2402, IP Authentication Header
RFC2403, The Use of HMAC-MD5-96 within ESP and AH
RFC2404, The Use of HMAC-SHA-1-96 within ESP and AH
RFC2405, The ESP DES-CBC Cipher Algorithm With Explicit IV
RFC2406, IP Encapsulating Security Payload (ESP)
RFC2407, The Internet IP Security Domain of Interpretation for ISAKMP
RFC2408, Internet Security Association and Key Management Protocol (ISAKMP)
RFC2409, The Internet Key Exchange (IKE)
RFC2410, The NULL Encryption Algorithm and Its Use With IPsec
RFC2411, IP Security Document Roadmap
RFC2412, The OAKLEY Key Determination Protocol
RFC2451, The ESP CBC-Mode Cipher Algorithms
RFC2104, HMAC: Keyed-Hashing for Message Authentication

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H