## CentreCOM AR550S 設定例集 2.9
##  152 CUGサービス（端末型）を利用した3拠点間IPsec接続（インターネット接続はセンタールーター経由）
##  ルーターAのコンフィグ
##
## 「#」で始まる行は、コンソールから入力しないと意味を持たないコマンドです。

ADD USER=secoff PASSWORD=PasswordS PRIVILEGE=SECURITYOFFICER
CREATE PPP=1 OVER=eth0-ANY
SET PPP=1 OVER=eth0-ANY BAP=OFF IPREQUEST=ON USER=user@isp PASSWORD=isppasswd LQR=OFF ECHO=ON
CREATE PPP=0 OVER=eth0-ANY
SET PPP=0 OVER=eth0-ANY BAP=OFF IPREQUEST=ON USER=userA PASSWORD=passwdA LQR=OFF ECHO=ON
ENABLE IP
ENABLE IP REMOTEASSIGN
ADD IP INT=vlan1 IP=192.168.10.1 MASK=255.255.255.0
ADD IP INT=ppp1 IP=0.0.0.0 MASK=0.0.0.0
ADD IP INT=ppp0 IP=10.1.1.1 MASK=255.255.255.255
ADD IP ROUTE=0.0.0.0 INT=ppp1 NEXTHOP=0.0.0.0
ADD IP ROUTE=10.0.0.0 MASK=255.0.0.0 INT=ppp0 NEXTHOP=0.0.0.0
ADD IP ROUTE=192.168.0.0 MASK=255.255.0.0 INT=ppp0 NEXTHOP=0.0.0.0
ENABLE FIREWALL
CREATE FIREWALL POLICY=net
ENABLE FIREWALL POLICY=net ICMP_F=PING,UNREACHABLE
DISABLE FIREWALL POLICY=net IDENTPROXY
ADD FIREWALL POLICY=net INT=vlan1 TYPE=PRIVATE
ADD FIREWALL POLICY=net INT=ppp0 TYPE=PRIVATE
ADD FIREWALL POLICY=net INT=ppp1 TYPE=PUBLIC
ADD FIREWALL POLICY=net NAT=ENHANCED INT=vlan1 GBLINT=ppp1
ADD FIREWALL POLICY=net NAT=ENHANCED INT=ppp0 GBLINT=ppp1
# CREATE ENCO KEY=1 TYPE=GENERAL VALUE="secret-ab"
# CREATE ENCO KEY=2 TYPE=GENERAL VALUE="secret-ac"
CREATE ISAKMP POLICY="i_B" PEER=10.1.1.2 KEY=1 SENDN=TRUE HEARTBEATMODE=BOTH
CREATE ISAKMP POLICY="i_C" PEER=10.1.1.3 KEY=2 SENDN=TRUE HEARTBEATMODE=BOTH
CREATE IPSEC SASPEC=1 KEYMAN=ISAKMP PROTOCOL=ESP ENCALG=DES HASHALG=SHA
CREATE IPSEC BUNDLE=1 KEYMAN=ISAKMP STRING="1"
CREATE IPSEC POLICY="isa" INT=ppp0 ACTION=PERMIT LPORT=500 RPORT=500 TRANSPORT=UDP
CREATE IPSEC POLICY="vpn_B" INT=ppp0 ACTION=IPSEC KEYMAN=ISAKMP BUNDLE=1 PEER=10.1.1.2
SET IPSEC POLICY="vpn_B" LAD=0.0.0.0 LMA=0.0.0.0 RAD=192.168.20.0 RMA=255.255.255.0
CREATE IPSEC POLICY="vpn_C" INT=ppp0 ACTION=IPSEC KEYMAN=ISAKMP BUNDLE=1 PEER=10.1.1.3
SET IPSEC POLICY="vpn_C" LAD=0.0.0.0 LMA=0.0.0.0 RAD=192.168.30.0 RMA=255.255.255.0
ENABLE IPSEC
ENABLE ISAKMP
# LOGIN secoff
# ENABLE SYSTEM SECURITY_MODE
