[index] CentreCOM AR550S コマンドリファレンス 2.9

# RESET PPP

カテゴリー：PPP / PPPインターフェース

`RESET PPP=ppp-interface [COUNTER] [LINKCOUNTER={ONLINE|INDATA|OUTDATA|TOTALDATA|ALL}]`

ppp-interface: PPPインターフェース番号（0〜511）

指定したPPPインターフェースをリセット、あるいは、インターフェースの一般統計カウンター、あるいは、通信量リミッター（INDATALIMIT、OUTDATALIMIT、UPTIMELIMIT、TOTALDATALIMIT）の通信カウンターをリセットする。

パラメーター

PPP: PPPインターフェース番号

COUNTER: 一般的な統計カウンターをリセットする。

LINKCOUNTER: 通信量リミッターが使用するカウンターをリセットする。

関連コマンド

CREATE PPP
DESTROY PPP
DISABLE PPP
ENABLE PPP
PURGE PPP
SET PPP
SHOW PPP LIMITS

参考

RFC1331, The Point-to-Point Protocol (PPP) for the Transmission of Multi-protocol Datagrams over Point-to-Point Links
RFC1332, The PPP Internet Protocol Control Protocol (IPCP)
RFC1333, PPP Link Quality Monitoring
RFC1334, PPP Authentication Protocols
RFC1548, The Point-to-Point Protocol (PPP)
RFC1549, PPP in HDLC Framing
RFC1570, PPP LCP Extensions
RFC1638, PPP Bridging Control Protocol (BCP)
RFC1661, The Point-to-Point Protocol (PPP)
RFC1662, PPP in HDLC-like Framing
RFC1877, PPP Internet Protocol Control Protocol Extensions for Name Server Addresses
RFC2516, A Method for Transmitting PPP Over Ethernet (PPPoE)

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H