[index] CentreCOM AR550S コマンドリファレンス 2.9

# SHOW PPP LIMITS

カテゴリー：PPP / PPPインターフェース

`SHOW PPP[=ppp-interface] LIMITS`

ppp-interface: PPPインターフェース番号（0〜511）

通信量リミッターの限度値と現在の累計値を表示する。

パラメーター

PPP: PPPインターフェース番号

入力・出力・画面例

    Manager > show ppp limits

    ppp0:
      Limit Counter           Current     Limit       Remaining   Previous
      ----------------------------------------------------------------------------
      Connection Time          0:00       Unlimited   --
      In Data                   0.0 MB    Unlimited   --
      Out Data                  0.0 MB    Unlimited   --
      Total Data                0.0 MB    Unlimited   --
      PADR Retry                0            15          15
      ----------------------------------------------------------------------------

表 1
Name | PPPインターフェース名
Connection Time | 累積通信時間（時間:分）
In Data | 累積受信量（MB）
Out Data | 累積送信量（MB）
Total Data | 累積通信量（送受信量）（MB）
PADR Retry | PADRの累計送信回数（累計値はPPPoEディスカバリーステージの間のみ変動し、PPPoEセッション確立後は常に0が表示される）
Current | 現在までの累計値。限度に達したときはEXCEEDEDと表示される
Limit | 設定されている限度値。設定していないとき（PADR Retryは設定が0のとき）はUnlimitedと表示される
Remaining | 限度値までの残り通信量/時間

関連コマンド

CREATE PPP TEMPLATE
RESET PPP
SET PPP

参考

RFC1331, The Point-to-Point Protocol (PPP) for the Transmission of Multi-protocol Datagrams over Point-to-Point Links
RFC1332, The PPP Internet Protocol Control Protocol (IPCP)
RFC1333, PPP Link Quality Monitoring
RFC1334, PPP Authentication Protocols
RFC1548, The Point-to-Point Protocol (PPP)
RFC1549, PPP in HDLC Framing
RFC1570, PPP LCP Extensions
RFC1638, PPP Bridging Control Protocol (BCP)
RFC1661, The Point-to-Point Protocol (PPP)
RFC1662, PPP in HDLC-like Framing
RFC1877, PPP Internet Protocol Control Protocol Extensions for Name Server Addresses
RFC2516, A Method for Transmitting PPP Over Ethernet (PPPoE)

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H