[index] CentreCOM AR550S コマンドリファレンス 2.9

# PURGE BGP DAMPING

カテゴリー：IP / 経路制御（BGP-4）

`PURGE BGP DAMPING`

BGP-4ルートフラップダンピングの設定情報をすべて削除する。
カスタムパラメーターセットやルートフラップの履歴情報は削除され、ルートフラップダンピング機能は無効化される。

備考・注意事項

ランタイムメモリー上にあるルートフラップダンピング関連の設定がすべて削除されるため、運用中のシステムで本コマンドを実行するときは十分に注意すること。

関連コマンド

ADD BGP PEER
CREATE BGP DAMPING PARAMETERSET
DESTROY BGP DAMPING PARAMETERSET
DISABLE BGP DAMPING
ENABLE BGP DAMPING
RESET BGP DAMPING
SET BGP DAMPING PARAMETERSET
SHOW BGP DAMPING
SHOW BGP DAMPING ROUTES

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2439, BGP Route Flap Damping
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H