[index] CentreCOM AR550S コマンドリファレンス 2.9

# ENABLE BGP DEFAULTORIGINATE

カテゴリー：IP / 経路制御（BGP-4）

`ENABLE BGP DEFAULTORIGINATE`

BGPの経路表にデフォルト経路（0.0.0.0/0）を取り込むようにする。デフォルトは取り込まない。
実際にデフォルト経路を取り込むには、本コマンドを実行するだけでなく、以下の設定が必要。
・デフォルト経路を静的に設定するか、他のルーティングプロトコル経由で学習できるよう設定する。
・ADD BGP IMPORTコマンドかADD BGP NETWORKコマンドを実行して、デフォルト経路がBGPの経路表に取り込まれるよう設定する。たとえば、ADD BGP IMPORT=STATIC、またはADD BGP NETWORK=0.0.0.0/0のように設定する。
なお、取り込んだデフォルト経路をBGPピアに通知するかどうかは、別途ADD BGP PEERコマンドのDEFAULTORIGINATEパラメーターで設定する（デフォルトは通知しない）。

関連コマンド

ADD BGP PEER
DISABLE BGP DEFAULTORIGINATE
SET BGP PEER

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2439, BGP Route Flap Damping
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H