[index] CentreCOM AR550S コマンドリファレンス 2.9

# ENABLE IPV6 DEBUG

カテゴリー：IPv6 / 一般コマンド

`ENABLE IPV6 DEBUG`

IPv6モジュールのデバッグ表示機能を有効にする。デフォルトは無効。

入力・出力・画面例

    Manager > enable ipv6 debug

    Info (1066271): IPv6 debuging has been enabled.

    Manager > IPV6_Send_To_Ethernet: outIpInd=1, outAddrInd=0
    IPV6_Send_To_Ethernet: nextHop=::
    IPV6_Send_To_Ethernet: destaddr=ff02::0009

    Manager > ipv6TunnelReceive: ipIndex=1
    ipv6TunnelReceive: ifIndex=5
    ipv6TunnelReceive: ipInd=1, logInd=0
    ipv6TunnelReceive: buf: ifInd=5, ipInd=1, logInd=0
    v6hdr: len=32, hop=255, prot=17, ver=1610612736
    src=3ffe:0b80:003c:0100::0001
    dest=ff02::0009
    IPV6_Receive: destaddr: ff02::0009 srcaddr:3ffe:0b80:003c:0100::0001
    IPV6_Receive: pktL=32, bufIpInd=2, bufLogInd=1, nH=17 localType = 5
    IPV6_Receive: addrIndex=1, intName=virt0, ifIntAddrNum=1 ipIntIndex=2
    local packet received

    Manager > ipv6TunnelSendPacket: tunneladd=3ffe:0b80:003c:0100::0002
    len=32, nH=17, hop=255
    ifInd=1, ipInd=1, ipLog=0
    dest=ff02::0009
    src=3ffe:0b80:003c:0100::0002
    prot=41, len=92
    src=172.16.20.254  , dest=172.16.10.1

    Manager > disable ipv6 debug

    Info (1066270): IPv6 debuging has been disabled.

備考・注意事項

本コマンドは、トラブルシューティング時など、内部情報の確認が必要な場合を想定したものですので、ご使用に際しては弊社技術担当にご相談ください。

関連コマンド

DISABLE IPV6 DEBUG
SHOW IPV6

参考

RFC2460, Internet Protocol, Version 6 (IPv6) Specification
RFC2461, Neighbor Discovery for IP Version 6 (IPv6)
RFC2462, IPv6 Stateless Address Autoconfiguration
RFC2463, Internet Control Message Protocol (ICMPv6) for the Internet Protocol Version 6 (IPv6) Specification

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H