[index] CentreCOM AR550S コマンドリファレンス 2.9

# DELETE BGP PEERTEMPLATE

カテゴリー：IP / 経路制御（BGP-4）

`DELETE BGP PEERTEMPLATE=1..30`

BGPピアテンプレートを削除する。該当テンプレートを使用していたピアとの通信パラメーターは、テンプレートの設定が引き継がれた状態となる。

パラメーター

PEERTEMPLATE: BGPピアテンプレート番号。

関連コマンド

ADD BGP PEER
ADD BGP PEERTEMPLATE
DELETE BGP PEER
DISABLE BGP PEER
ENABLE BGP PEER
RESET BGP PEER
SET BGP PEER
SET BGP PEERTEMPLATE
SHOW BGP PEER
SHOW BGP PEERTEMPLATE

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2439, BGP Route Flap Damping
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H