[index] CentreCOM AR550S コマンドリファレンス 2.9

# SHOW ISAKMP

カテゴリー：IPsec / ISAKMP

`SHOW ISAKMP`

ISAKMPモジュールの情報を表示する。

入力・出力・画面例

    SecOff > show isakmp

    ISAKMP Module Configuration

      Module Status .......................... ENABLED
      UDP Port ............................... 500
      Debug Flag ............................. 00000000
      Global Debug Device .................... 0
      Local RSA Key .......................... -
      VPN Client Policy Server Enabled ....... FALSE
      VPN Client Policy File Name ............

表 1
Module Status | ISAKMPモジュールの有効・無効
UDP Port | ISAKMPメッセージの送受信に使うUDPポート
Debug Flag | 各デバッグオプションの有効・無効を示すビット列。数字は一番左から、パケットデバッグ（第0ビット）、状態遷移デバッグ（第1ビット）、トレースデバッグ（第3ビット）。値0は無効、値1は有効
Global Debug Device | デバッグ情報の出力先ポート番号
Local RSA key | デフォルトのRSA秘密鍵番号
VPN Client Policy Server Enabled | セキュリティーポリシーサーバー機能の有効・無効
VPN Client Policy File Name | クライアントに送信するデフォルトのセキュリティーポリシーファイル名

関連コマンド

DISABLE ISAKMP
ENABLE ISAKMP

参考

RFC2401, Security Architecture for the Internet Protocol
RFC2402, IP Authentication Header
RFC2403, The Use of HMAC-MD5-96 within ESP and AH
RFC2404, The Use of HMAC-SHA-1-96 within ESP and AH
RFC2405, The ESP DES-CBC Cipher Algorithm With Explicit IV
RFC2406, IP Encapsulating Security Payload (ESP)
RFC2407, The Internet IP Security Domain of Interpretation for ISAKMP
RFC2408, Internet Security Association and Key Management Protocol (ISAKMP)
RFC2409, The Internet Key Exchange (IKE)
RFC2410, The NULL Encryption Algorithm and Its Use With IPsec
RFC2411, IP Security Document Roadmap
RFC2412, The OAKLEY Key Determination Protocol
RFC2451, The ESP CBC-Mode Cipher Algorithms
RFC2104, HMAC: Keyed-Hashing for Message Authentication

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H