[index] CentreCOM AR550S コマンドリファレンス 2.9

# ADD SNMP GROUP

カテゴリー：運用・管理 / SNMP

`ADD SNMP GROUP=group SECURITYLEVEL={noAuthNoPriv|authNoPriv|authPriv} [READVIEW=view] [WRITEVIEW=view] [NOTIFYVIEW=view]`

group: SNMPグループ名（1〜32文字。大文字小文字を区別する）
view: SNMPビュー名（1〜32文字。大文字小文字を区別する）

（SNMPv3）ユーザーグループを定義する。
グループ名とセキュリティーレベルの組み合わせは一意でなくてはならない。

パラメーター

GROUP: SNMPグループ名

SECURITYLEVEL: 本グループ所属のユーザーに求められる最低限のセキュリティーレベルを指定する。noAuthNoPriv（認証なし・暗号化なし）、authNoPriv（認証あり・暗号化なし）、authPriv（認証あり・暗号化あり）から選択する。

READVIEW: 本グループ所属のユーザーが読み出せるMIBオブジェクトの範囲（ビュー）を指定する。ビューはADD SNMP VIEWコマンドで定義する。READVIEWの指定がない場合、本グループ所属のユーザーはいかなるMIBオブジェクトも読み出せない。

WRITEVIEW: 本グループ所属のユーザーが書き込めるMIBオブジェクトの範囲（ビュー）を指定する。ビューはADD SNMP VIEWコマンドで定義する。WRITEVIEWの指定がない場合、本グループ所属のユーザーはいかなるMIBオブジェクトにも書き込めない。

NOTIFYVIEW: 本グループ所属のユーザーが受け取れる通知MIBオブジェクトの範囲（ビュー）を指定する。ビューはADD SNMP VIEWコマンドで定義する。NOTIFYVIEWの指定がない場合、本グループ所属のユーザーはいかなる通知MIBオブジェクトも受け取れない。

例

``■ SNMPグループ「admins」を定義する。セキュリティーレベルはauthPriv（認証あり・暗号化あり）。読み出し、書き込み、通知受信のすべてにおいて、internetノード（1.3.6.1）以下のすべてのオブジェクトにアクセスできるよう設定する。
`ADD SNMP VIEW=most MIB=internet TYPE=INCLUDE
ADD SNMP GROUP=admins SECURITYLEVEL=authPriv READVIEW=most WRITEVIEW=most NOTIFYVIEW=most
` ■ SNMPグループ「mib2operators」を定義する。セキュリティーレベルはauthNoPriv（認証あり・暗号化なし）。mib-2ノード（1.3.6.1.2.1）以下の読み出しだけを許可する。
`ADD SNMP VIEW=standard MIB=mib-2 TYPE=INCLUDE
ADD SNMP GROUP=mib2operators SECURITYLEVEL=authNoPriv READVIEW=standard`

関連コマンド

ADD SNMP USER
ADD SNMP VIEW
DELETE SNMP GROUP
SET SNMP GROUP
SHOW SNMP
SHOW SNMP GROUP
SHOW SNMP USER
SHOW SNMP VIEW

参考

RFC1155, Structure and Identification of Management Information for TCP/IP-based Internets
RFC1157, A Simple Network Management Protocol (SNMP)
RFC1213, Management Information Base for Network Management of TCP/IP-based internets: MIB-II
RFC1239, Reassignment of Experimental MIBs to Standard MIBs
RFC1398, Definitions of Managed Objects for the Ethernet-like Interface Types
RFC1493, Definitions of Managed Objects for Bridges
RFC1514, Host Resources MIB
RFC1573, Evolution of the Interfaces Group of MIB-II
RFC1901, Introduction to Community-based SNMPv2
RFC1902, Structure of Management Information for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1903, Textual Conventions for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1904, Conformance Statements for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1905, Protocol Operations for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1906, Transport Mappings for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1907, Management Information Base for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC2233, The Interfaces Group MIB using SMIv2
RFC2576, Coexistence between Version 1, Version 2, and Version 3 of the Internet-standard Network Management Framework
RFC2578, Structure of Management Information Version 2 (SMIv2)
RFC2579, Textual Conventions for SMIv2
RFC2580, Conformance Statements for SMIv2
RFC3410, Introduction and Applicability Statements for Internet Standard Management Framework
RFC3411, An Architecture for Describing Simple Network Management Protocol (SNMP) Management Frameworks
RFC3412, Message Processing and Dispatching for the Simple Network Management Protocol (SNMP)
RFC3413, Simple Network Management Protocol (SNMP) Applications
RFC3414, User-based Security Model (USM) for version 3 of the Simple Network Management Protocol (SNMPv3)
RFC3415, View-based Access Control Model (VACM) for the Simple Network Management Protocol (SNMP)
RFC3416, Version 2 of the Protocol Operations for the Simple Network Management Protocol (SNMP)
RFC3417, Transport Mappings for the Simple Network Management Protocol (SNMP)
RFC3418, Management Information Base (MIB) for the Simple Network Management Protocol (SNMP)

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H