[index] CentreCOM AR550S コマンドリファレンス 2.9

# SET PPP DNSPRIMARY

カテゴリー：PPP / 一般コマンド

`SET PPP [DNSPRIMARY=ipadd] [DNSSECONDARY=ipadd] [WINSPRIMARY=ipadd] [WINSSECONDARY=ipadd]`

ipadd: IPアドレス

IPCPで相手に通知するプライマリー/セカンダリーDNSサーバーアドレス、プライマリー/セカンダリーWINSサーバーアドレスを設定する。
ここでの設定はすべてのPPPインターフェースに適用される。

パラメーター

DNSPRIMARY: プライマリーDNS（Domain Name Service）サーバーのIPアドレス。IPCPネゴシエーション時に、IP-Primary-DNS-Server-Addressオプションで相手側に送られる。

DNSSECONDARY: セカンダリーDNS（Domain Name Service）サーバーのIPアドレス。IPCPネゴシエーション時に、IP-Secondary-DNS-Server-Addressオプションで相手側に送られる。

WINSPRIMARY: プライマリーWINS（Windows Internet Name Service）サーバーのIPアドレス。IPCPネゴシエーション時に、IP-Primary-NBNS-Server-Addressオプションで相手側に送られる。

WINSSECONDARY: セカンダリーWINS（Windows Internet Name Service）サーバーのIPアドレス。IPCPネゴシエーション時に、IP-Secondary-NBNS-Server-Addressオプションで相手側に送られる。

関連コマンド

SHOW PPP NAMESERVERS

参考

RFC1331, The Point-to-Point Protocol (PPP) for the Transmission of Multi-protocol Datagrams over Point-to-Point Links
RFC1332, The PPP Internet Protocol Control Protocol (IPCP)
RFC1333, PPP Link Quality Monitoring
RFC1334, PPP Authentication Protocols
RFC1548, The Point-to-Point Protocol (PPP)
RFC1549, PPP in HDLC Framing
RFC1570, PPP LCP Extensions
RFC1638, PPP Bridging Control Protocol (BCP)
RFC1661, The Point-to-Point Protocol (PPP)
RFC1662, PPP in HDLC-like Framing
RFC1877, PPP Internet Protocol Control Protocol Extensions for Name Server Addresses
RFC2516, A Method for Transmitting PPP Over Ethernet (PPPoE)

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H