## CentreCOM AR550S 設定例集 2.9
##  106 L2TPによるリモートアクセス型LAN間接続（ファイアウォールあり）
##  ルーターA(LAC)のコンフィグ

ENABLE L2TP
ENABLE L2TP SERVER=BOTH
ADD L2TP CALL=REMOTE IP=200.100.10.1 TYPE=VIRTUAL PRECEDENCE=OUT PASSWORD=l2tpB
CREATE PPP=0 OVER=eth0-ANY IPREQUEST=ON
SET PPP=0 OVER=eth0-ANY BAP=OFF USERNAME="user@ispA" PASSWORD="isppasswdA" LQR=OFF ECHO=ON
CREATE PPP=1 OVER=TNL-REMOTE BAP=OFF IDLE=ON IPREQUEST=ON LQR=OFF
SET PPP=1 USER=AAA PASSWORD=PasswordA
ENABLE IP
ENABLE IP REMOTEASSIGN
ADD IP INT=vlan1 IP=192.168.10.1 MASK=255.255.255.0
ADD IP INT=ppp0 IP=0.0.0.0
ADD IP INT=ppp1 IP=0.0.0.0
ADD IP ROUTE=0.0.0.0 INT=ppp0 NEXT=0.0.0.0
ADD IP ROUTE=192.168.20.0 MASK=255.255.255.0 INT=ppp1 NEXT=0.0.0.0
ENABLE FIREWALL
CREATE FIREWALL POLICY=NET
ENABLE FIREWALL POLICY=NET ICMP_F=PING,UNREACH
DISABLE FIREWALL POLICY=NET IDENTPROXY
ADD FIREWALL POLICY=NET INT=vlan1 TYPE=PRIVATE
ADD FIREWALL POLICY=NET INT=ppp0 TYPE=PUBLIC
ADD FIREWALL POLICY=NET INT=ppp1 TYPE=PUBLIC
ADD FIREWALL POLICY=NET NAT=ENHANCED INT=vlan1 GBLINT=ppp1
ADD FIREWALL POLICY=NET NAT=ENHANCED INT=vlan1 GBLINT=ppp0
