## CentreCOM AR550S 設定例集 2.9
##  41 PPPoEマルチセッションによる端末型インターネット接続（IPプロトコルに基づくポリシールーティング）
##  ルーターのコンフィグ

CREATE PPP=0 OVER=eth0-ispA
SET PPP=0 OVER=eth0-ispA USER=user@ispA PASSWORD=isppasswdA LQR=OFF BAP=OFF ECHO=ON
CREATE PPP=0 OVER=eth0-ispB
SET PPP=1 OVER=eth0-ispB USER=user@ispB PASSWORD=isppasswdB LQR=OFF BAP=OFF ECHO=ON
ENABLE IP
ADD IP FILTER=1 TYPE=POLICY SO=192.168.10.0 SM=255.255.255.0 PROTOCOL=TCP DPORT=80 POLICY=1
ADD IP FILTER=1 TYPE=POLICY SO=0.0.0.0 POLICY=2
ADD IP INT=vlan1 IP=192.168.10.1 MASK=255.255.255.0 POLICYFILTER=1
ADD IP ROUTE=0.0.0.0 MASK=0.0.0.0 INTERFACE=ppp1 NEXT=0.0.0.0 POLICY=1
ADD IP ROUTE=0.0.0.0 MASK=0.0.0.0 INTERFACE=ppp0 NEXT=0.0.0.0 POLICY=2
ENABLE FIREWALL
CREATE FIREWALL POLICY=net
ENABLE FIREWALL POLICY=net ICMP_F=PING,UNREACHABLE
DISABLE FIREWALL POLICY=net IDENTPROXY
ADD FIREWALL POLICY=net INT=vlan1 TYPE=PRIVATE
ADD FIREWALL POLICY=net INT=ppp0 TYPE=PUBLIC
ADD FIREWALL POLICY=net INT=ppp1 TYPE=PUBLIC
ADD FIREWALL POLICY=net NAT=ENHANCED INT=vlan1 GBLINT=ppp0
ADD FIREWALL POLICY=net NAT=ENHANCED INT=vlan1 GBLINT=ppp1
