[index] CentreCOM 8700SLシリーズ コマンドリファレンス 2.9

# SHOW PPP DEBUG

カテゴリー：PPP / PPPインターフェース

`SHOW PPP[=ppp-interface] DEBUG`

ppp-interface: PPPインターフェース番号（0〜511）

現在有効なデバッグオプションを表示する。

パラメーター

PPP: PPPインターフェース番号

入力・出力・画面例

    Manager > show ppp=0 debug

      Interface        Enabled Debug Modes
      ----------------------------------------------------------------------------
      ppp0             LCP, NCP
      ----------------------------------------------------------------------------

表 1
Interface | インターフェース名
Enabled Debug Modes | 有効なデバッグオプション（AUTH、DEMAND、LCP、NCP、PKT、UTILISATION）

参考

RFC1331, The Point-to-Point Protocol (PPP) for the Transmission of Multi-protocol Datagrams over Point-to-Point Links
RFC1332, The PPP Internet Protocol Control Protocol (IPCP)
RFC1333, PPP Link Quality Monitoring
RFC1334, PPP Authentication Protocols
RFC1548, The Point-to-Point Protocol (PPP)
RFC1549, PPP in HDLC Framing
RFC1570, PPP LCP Extensions
RFC1638, PPP Bridging Control Protocol (BCP)
RFC1661, The Point-to-Point Protocol (PPP)
RFC1662, PPP in HDLC-like Framing
RFC1877, PPP Internet Protocol Control Protocol Extensions for Name Server Addresses
RFC2516, A Method for Transmitting PPP Over Ethernet (PPPoE)

(C) 2003 - 2010 アライドテレシスホールディングス株式会社

PN: J613-M0019-01 Rev.P