[index] CentreCOM 8700SLシリーズ コマンドリファレンス 2.9

# SHOW IP COMMUNITYLIST

カテゴリー：IP / 経路制御（BGP-4）
備考：フィーチャーライセンス AT-FL-08 が必要

`SHOW IP COMMUNITYLIST[=1..99] [OLDCOMMUNITYFORMAT]`

コミュニティーリストの情報を表示する。

パラメーター

COMMUNITYLIST: コミュニティーリスト番号。省略時は有効なエントリーを持つすべてのリストが表示される。

OLDCOMMUNITYFORMAT: コミュニティー番号を古い形式で表示させるときに指定する。本オプション指定時は、コミュニティー番号がasn:xxxの形式ではなく、単一の32ビット整数値として表示される。

入力・出力・画面例

    Manager > show ip communitylist
    IP Community lists

    List  Entry       Community List
    ------------------------------------------------------------
    1     1           Exclude 65003:100
          2           Include internet
    ------------------------------------------------------------

表 1
List | コミュニティーリスト番号
Entry | エントリー番号
Community list | マッチ条件（コミュニティーのリスト）とマッチ時のアクション

関連コマンド

ADD IP COMMUNITYLIST
DELETE IP COMMUNITYLIST

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2003 - 2010 アライドテレシスホールディングス株式会社

PN: J613-M0019-01 Rev.P