[index] CentreCOM 8700SLシリーズ コマンドリファレンス 2.9

# SET IP PREFIXLIST

カテゴリー：IP / 経路制御（BGP-4）
備考：フィーチャーライセンス AT-FL-08 が必要

`SET IP PREFIXLIST=plist ENTRY=1..65535 [ACTION={MATCH|NOMATCH}] [PREFIX=ipadd] [MASKLENGTH=plen[-plen]]`

plist: プレフィックスリスト名（0〜15文字。英数字とアンダースコアを使用可能。大文字小文字を区別する）
ipadd: IPアドレス
plen: プレフィックス長（0〜32ビット）

プレフィックスリストエントリーの設定を変更する。

パラメーター

PREFIXLIST: プレフィックスリスト名

ENTRY: リスト内におけるエントリーの位置。必須パラメーター。

ACTION: 比較対象のプレフィックスが本エントリーにマッチした場合に返す結果の値（MATCHかNOMATCH）。省略時はMATCHとなる。

PREFIX: プレフィックス（宛先ネットワークアドレス）。

MASKLENGTH: プレフィックス長。ハイフン区切りで範囲指定も可能。省略時はPREFIXパラメーターで指定したプレフィックスのクラス標準マスク長となる（PREFIX=0.0.0.0のときは0になる）。

関連コマンド

ADD BGP PEER
ADD IP PREFIXLIST
ADD IP ROUTEMAP
DELETE IP PREFIXLIST
SET BGP PEER
SHOW IP PREFIXLIST

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2003 - 2010 アライドテレシスホールディングス株式会社

PN: J613-M0019-01 Rev.P