[index] CentreCOM 8700SLシリーズ コマンドリファレンス 2.9

# ADD BGP IMPORT

カテゴリー：IP / 経路制御（BGP-4）
備考：フィーチャーライセンス AT-FL-08 が必要

`ADD BGP IMPORT={OSPF|RIP|STATIC|INTERFACE} [ROUTEMAP[=routemap]]`

routemap: ルートマップ名（0〜15文字。英数字とアンダースコアを使用可能。大文字小文字を区別する）

BGPで配布する経路情報のソース（インターフェース経路、静的経路、RIP、OSPF）を指定する。
オプションでルートマップを使えば、経路情報をBGPにインポートする際にフィルタリングや属性の設定を行うこともできる。

パラメーター

IMPORT: BGPに取り込む経路情報のソース（起源）。INTERFACEはインターフェース（ダイレクト）経路、STATICはインターフェース経路を除く静的経路、RIPはRIP経路、OSPFはOSPF経路を示す。

ROUTEMAP: インポート時に適用するルートマップ。MATCH節はNEXTHOP、ORIGIN、PREFIXLIST、TAGだけを使用できる。SET節はすべて使用可能。デフォルトはなし。

例

``■ インターフェース経路と静的経路をBGPで配布する。
`ADD BGP IMPORT=INTERFACE
ADD BGP IMPORT=STATIC
` ■ OSPF起源の経路情報をBGPで使用する。インポート時にはルートマップ「ospf_import」を使って、フィルタリングと属性設定を行う。
`ADD BGP IMPORT=OSPF ROUTEMAP=ospf_import`

関連コマンド

ADD IP ROUTEMAP
DELETE BGP IMPORT
SET BGP IMPORT
SHOW BGP IMPORT

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2003 - 2010 アライドテレシスホールディングス株式会社

PN: J613-M0019-01 Rev.P