[index] CentreCOM 8700SLシリーズ コマンドリファレンス 2.9

# ENABLE IPV6 DEBUG

カテゴリー：IPv6 / 一般コマンド
備考：フィーチャーライセンス AT-FL-13 が必要

`ENABLE IPV6 DEBUG`

IPv6モジュールのデバッグ表示機能を有効にする。デフォルトは無効。

入力・出力・画面例

    Manager > enable ipv6 debug

    Info (1066271): IPv6 debuging has been enabled.

    Manager > Sending to Vlan: outIpIndex=2, outAddrIndex=0
    Sending to Vlan: nextHop=::
    Sending to Vlan: destAddress=ff02::0009 portNumber=0
    calling vlanDataRequest on all ports
    Sending to Vlan: outIpIndex=1, outAddrIndex=0
    Sending to Vlan: nextHop=::
    Sending to Vlan: destAddress=ff02::0009 portNumber=0
    calling vlanDataRequest on all ports

    Manager > Received IPv6 pkt: DestAddress: ff02::0009
     SrcAddress:fe80::0200:f4ff:fec4:0463
    Received IPv6 pkt: pktL=32, bufIpInd=1, bufLogInd=0, nH=17 localType = 524288
    Received IPv6 pkt: addrIndex=0, intName=vlan10, ifIntAddrNum=2 ipIntIndex=1
    iplocaltype=0
    Local packet received

    Manager > Received IPv6 pkt: DestAddress: 3ffe:0b80:003c:0020:0290:99ff:fe0e:e00
    a
     SrcAddress:3ffe:0b80:003c:0010:0290:99ff:fe42:00f2
    Received IPv6 pkt: pktL=16, bufIpInd=1, bufLogInd=1, nH=58 localType = 0
    Received IPv6 pkt: addrIndex=1, intName=vlan10, ifIntAddrNum=2 ipIntIndex=1
    iplocaltype=0
    Forwarding IPv6 pkt: ipInterface=2, addIndex=1
    nexthop=::
    dest=3ffe:0b80:003c:0020::
    Sending to Vlan: outIpIndex=2, outAddrIndex=1
    Sending to Vlan: nextHop=::
    Sending to Vlan: destAddress=3ffe:0b80:003c:0020:0290:99ff:fe0e:e00a portNumber=
    0
    Don't know how to send, creating VLan NDCache entry
    int=2, m=1, srcLink=00-00-cd-08-17-0c
    destAddr=ff02::0001:ff0e:e00a
    ndAddr=3ffe:0b80:003c:0020:0290:99ff:fe0e:e00a
    multicast=1
    dest=ff02::0001:ff0e:e00a
    Sending to Vlan: outIpIndex=2, outAddrIndex=1
    Sending to Vlan: nextHop=::
    Sending to Vlan: destAddress=ff02::0001:ff0e:e00a portNumber=0
    calling vlanDataRequest on all ports

備考・注意事項

本コマンドは、トラブルシューティング時など、内部情報の確認が必要な場合を想定したものですので、ご使用に際しては弊社技術担当にご相談ください。

関連コマンド

DISABLE IPV6 DEBUG
SHOW IPV6

参考

RFC2460, Internet Protocol, Version 6 (IPv6) Specification
RFC2461, Neighbor Discovery for IP Version 6 (IPv6)
RFC2462, IPv6 Stateless Address Autoconfiguration
RFC2463, Internet Control Message Protocol (ICMPv6) for the Internet Protocol Version 6 (IPv6) Specification

(C) 2003 - 2010 アライドテレシスホールディングス株式会社

PN: J613-M0019-01 Rev.P