[index] CentreCOM 8700SLシリーズ コマンドリファレンス 2.9

# ENABLE PING POLL DEBUG

カテゴリー：IP / Pingポーリング

`ENABLE PING POLL=poll-id DEBUG`

poll-id: PingポーリングID（1〜100）

Pingポーリングのデバッグ表示を有効にする。デフォルトは無効。

パラメーター

POLL: PingポーリングID

入力・出力・画面例

    Manager > enable ping poll=1 debug

    Info (1058003): Operation successful.

    Manager > Ping Poll(1): Sending Ping to 172.17.28.100

    Manager > Ping Poll(1): Received a ping reply from 172.17.28.100
    Ping Poll(1): State=UP upCount=33(30) failCount=0(5/5)

    Manager > Ping Poll(1): Sending Ping to 172.17.28.100

    Manager > Ping Poll(1): Received no reply from 172.17.28.100
    Ping Poll(1): State=UP upCount=0(30) failCount=1(5/5)

    Manager > Ping Poll(1): Sending Ping to 172.17.28.100

    Manager > Ping Poll(1): Received no reply from 172.17.28.100
    Ping Poll(1): State=UP upCount=0(30) failCount=2(5/5)
    Ping Poll(1): Sending Ping to 172.17.28.100

    Manager > Ping Poll(1): Received no reply from 172.17.28.100
    Ping Poll(1): State=UP upCount=0(30) failCount=3(5/5)
    Ping Poll(1): Sending Ping to 172.17.28.100

    Manager > Ping Poll(1): Received no reply from 172.17.28.100
    Ping Poll(1): State=UP upCount=0(30) failCount=4(5/5)
    Ping Poll(1): Sending Ping to 172.17.28.100

    Manager > Ping Poll(1): Received no reply from 172.17.28.100
    Ping Poll(1): State=UP upCount=0(30) failCount=5(5/5)
    Ping Poll(1): Old State=UP New State=DOWN
    Ping Poll(1): Down Trigger
    Ping Poll(1): Sending Ping to 172.17.28.100

    Manager > Ping Poll(1): Received no reply from 172.17.28.100
    Ping Poll(1): State=DOWN upCount=0(30) failCount=5(5/5)
    Ping Poll(1): Sending Ping to 172.17.28.100

    ...

    Manager > Ping Poll(1): Received a ping reply from 172.17.28.100
    Ping Poll(1): State=DOWN upCount=1(30) failCount=4(5/5)
    Ping Poll(1): Sending Ping to 172.17.28.100

    Manager > Ping Poll(1): Received a ping reply from 172.17.28.100
    Ping Poll(1): State=DOWN upCount=2(30) failCount=3(5/5)
    Ping Poll(1): Sending Ping to 172.17.28.100

    ...

    Manager > Ping Poll(1): Received a ping reply from 172.17.28.100
    Ping Poll(1): State=DOWN upCount=29(30) failCount=0(5/5)
    Ping Poll(1): Sending Ping to 172.17.28.100

    Manager > Ping Poll(1): Received a ping reply from 172.17.28.100
    Ping Poll(1): State=DOWN upCount=30(30) failCount=0(5/5)
    Ping Poll(1): Old State=DOWN New State=UP
    Ping Poll(1): Up Trigger
    Ping Poll(1): Sending Ping to 172.17.28.100

    Manager > Ping Poll(1): Received a ping reply from 172.17.28.100
    Ping Poll(1): State=UP upCount=31(30) failCount=0(5/5)

備考・注意事項

本コマンドは、トラブルシューティング時など、内部情報の確認が必要な場合を想定したものですので、ご使用に際しては弊社技術担当にご相談ください。

関連コマンド

DISABLE PING POLL DEBUG
SHOW PING POLL

参考

RFC791, INTERNET PROTOCOL
RFC792, INTERNET CONTROL MESSAGE PROTOCOL
RFC950, Internet Standard Subnetting Procedure
RFC2460, Internet Protocol, Version 6 (IPv6) Specification
RFC2463, Internet Control Message Protocol (ICMPv6) for the Internet Protocol Version 6 (IPv6) Specification

(C) 2003 - 2010 アライドテレシスホールディングス株式会社

PN: J613-M0019-01 Rev.P