[index] CentreCOM 8700SLシリーズ コマンドリファレンス 2.9

# SET BGP IMPORT

カテゴリー：IP / 経路制御（BGP-4）
備考：フィーチャーライセンス AT-FL-08 が必要

`SET BGP IMPORT={OSPF|RIP|STATIC|INTERFACE} [ROUTEMAP[=routemap]]`

routemap: ルートマップ名（0〜15文字。英数字とアンダースコアを使用可能。大文字小文字を区別する）

BGPに経路情報を取り込むときに適用するルートマップを変更する。

パラメーター

IMPORT: BGPに取り込む経路情報のソース（起源）。

ROUTEMAP: インポート時に適用するルートマップ。MATCH節はNEXTHOP、ORIGIN、PREFIXLIST、TAGだけを使用できる。SET節はすべて使用可能。ルートマップを解除するときは、ルートマップ名を指定せず、単に「ROUTEMAP」と指定する。

関連コマンド

ADD BGP IMPORT
DELETE BGP IMPORT
SHOW BGP IMPORT

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2003 - 2010 アライドテレシスホールディングス株式会社

PN: J613-M0019-01 Rev.P