[index] CentreCOM 8700SLシリーズ コマンドリファレンス 2.9

# SHOW IP ROUTEMAP

カテゴリー：IP / 経路制御（BGP-4）
備考：フィーチャーライセンス AT-FL-08 が必要

`SHOW IP ROUTEMAP[=routemap] [OLDCOMMUNITYFORMAT]`

routemap: ルートマップ名（0〜15文字。英数字とアンダースコアを使用可能。大文字小文字を区別する）

ルートマップの情報を表示する。

パラメーター

ROUTEMAP: ルートマップ名。省略時はすべてのルートマップが表示される。

OLDCOMMUNITYFORMAT: コミュニティー番号を古い形式で表示させるときに指定する。本オプション指定時は、コミュニティー番号がasn:xxxの形式ではなく、単一の32ビット整数値として表示される。

入力・出力・画面例

    Manager > show ip routemap
    IP route Maps

    Map Name
      Entry       Action
          Clauses
    ------------------------------------------------------------
    color_slow_path
      1           Include
             set   Community   65010:1000 Add=no
    ------------------------------------------------------------
    add_myasn_twice
      1           Include
           match   Community   1 Exact=no
             set   AS-path     65010 65010
    ------------------------------------------------------------

表 1
Map name | ルートマップ名
Entry | エントリー番号
Action | エントリーのアクション
Clauses | SET節、MATCH節の設定内容。MATCH節はマッチ条件。SET節は許可（INCLUDE）された経路エントリーに対する属性設定の内容

関連コマンド

ADD IP ROUTEMAP
DELETE IP ROUTEMAP
SET IP ROUTEMAP

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2003 - 2010 アライドテレシスホールディングス株式会社

PN: J613-M0019-01 Rev.P