[index] CentreCOM 8700SLシリーズ コマンドリファレンス 2.9

# ADD BGP CONFEDERATIONPEER

カテゴリー：IP / 経路制御（BGP-4）
備考：フィーチャーライセンス AT-FL-08 が必要

`ADD BGP CONFEDERATIONPEER=1..65534`

コンフェデレーションEBGPピアのサブAS番号を指定する。
自分が所属するASコンフェデレーションの番号は、SET BGPコマンドのCONFEDERATIONIDパラメーターで設定する。また、自分が所属するサブAS（メンバーAS）番号は、SET IP AUTONOMOUSコマンドで設定する。

パラメーター

CONFEDERATIONPEER: コンフェデレーションEBGPピアが所属するサブASの番号。自サブAS番号やASコンフェデレーションIDと別の番号でなくてはならない。

例

``■ 「192.168.100.2」とコンフェデレーションEBGPセッションを張る。両者が所属するコンフェデレーションのAS番号は8686。自分が所属するサブAS番号は10、相手のサブAS番号は20とする。
`SET IP AUTONOMOUS=10
SET BGP CONFEDERATIONID=8686
ADD BGP PEER=192.168.100.2 REMOTEAS=20
ADD BGP CONFEDERATIONPEER=20
ENABLE BGP PEER=192.168.100.2`

備考・注意事項

コンフェデレーションに所属しているすべてのASを指定する必要はない。C-EBGPセッションを張っているピアのサブAS番号だけを指定すればよい。

関連コマンド

ADD BGP PEER
DELETE BGP CONFEDERATIONPEER
SET BGP
SET IP AUTONOMOUS
SHOW BGP CONFEDERATION

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2003 - 2010 アライドテレシスホールディングス株式会社

PN: J613-M0019-01 Rev.P