[index] CentreCOM 8700SLシリーズ コマンドリファレンス 2.9

# DELETE BGP NETWORK

カテゴリー：IP / 経路制御（BGP-4）
備考：フィーチャーライセンス AT-FL-08 が必要

`DELETE BGP NETWORK=prefix [MASK=ipadd]`

prefix: プレフィックス（IPアドレス/プレフィックス長）
ipadd: IPアドレスまたはネットマスク

BGPで配布するネットワークプレフィックスを削除する。
本コマンドを実行すると、BGP経路表から該当プレフィックス（登録されている場合）が削除され、すべてのBGPピアに対し、該当プレフィックスの取り消し（Withdraw）が通知される。

パラメーター

NETWORK: プレフィックス。ネットワークアドレスとプレフィックス長で指定する。プレフィックス長はMASKパラメーターで指定することも可能。

MASK: NETWORKで指定したネットワークアドレスに対するプレフィックスの有効長。

関連コマンド

ADD BGP NETWORK
SHOW BGP NETWORK
SHOW BGP ROUTE

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2003 - 2010 アライドテレシスホールディングス株式会社

PN: J613-M0019-01 Rev.P