[index] CentreCOM 8700SLシリーズ コマンドリファレンス 2.9

# ADD BGP NETWORK

カテゴリー：IP / 経路制御（BGP-4）
備考：フィーチャーライセンス AT-FL-08 が必要

`ADD BGP NETWORK=prefix [MASK=ipadd] [ROUTEMAP[=routemap]]`

prefix: プレフィックス（IPアドレス/プレフィックス長）
ipadd: IPアドレスまたはネットマスク
routemap: ルートマップ名（0〜15文字。英数字とアンダースコアを使用可能。大文字小文字を区別する）

BGPで配布するネットワークプレフィックスを指定する。
ルーターの経路表に本コマンドで指定したプレフィックスが追加された場合（静的設定やRIP、OSPFなどによる）、同プレフィックスはBGP経路表にもインポートされる。
オプションでルートマップを使えば、経路情報をBGPにインポートする際にフィルタリングや属性の設定を行うこともできる。

パラメーター

NETWORK: プレフィックス。ネットワークアドレスとプレフィックス長で指定する。プレフィックス長はMASKパラメーターで指定することも可能。

MASK: NETWORKで指定したネットワークアドレスに対するプレフィックスの有効長。

ROUTEMAP: ルートマップ名。該当プレフィックスに対するフィルタリングや通知時の属性設定に用いる。MATCH節はNEXTHOP、ORIGIN、PREFIXLIST、TAGだけを使用できる。SET節はすべて使用可能。

例

``■ プレフィックス192.168.100.0/24をBGPで配布する。
`ADD BGP NETWORK=192.168.100.0/24`

備考・注意事項

本コマンドで指定したプレフィックスが外部に通知されるのは、ルーターの経路表に該当プレフィックスが登録されている間だけであることに注意。

関連コマンド

DELETE BGP NETWORK
SHOW BGP NETWORK
SHOW BGP ROUTE

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2003 - 2010 アライドテレシスホールディングス株式会社

PN: J613-M0019-01 Rev.P