[index] CentreCOM 8948XL コマンドリファレンス 2.9

# SHOW BGP CONFEDERATION

カテゴリー：IP / 経路制御（BGP-4）
備考：フィーチャーライセンス AT-FL-09 が必要

`SHOW BGP CONFEDERATION`

ASコンフェデレーションの設定情報を表示する。

入力・出力・画面例

    Manager > show bgp confederation

    BGP confederation information

    Local AS ................ 65011
    Confederation ID ........ 65001
    Confederation peers ..... 65012
    Peers ................... 172.28.28.7 (AS 65003, EBGP)
                              172.28.28.8 (AS 65012, CBGP)

表 1
Local AS | 自AS番号
Confederation ID | 所属するコンフェデレーションのAS番号
Confederation peers | 上記コンフェデレーションに所属する他ASの一覧
Peers | BGPピアの一覧。IPアドレス（AS番号, BGPピアの種類）の形式。BGPピアの形式は、EBGP（E-BGPピア）、IBGP（I-BGPピア）、CBGP（コンフェデレーションE-BGPピア）のいずれか

関連コマンド

ADD BGP CONFEDERATIONPEER
DELETE BGP CONFEDERATIONPEER
SET BGP
SET IP AUTONOMOUS
SHOW BGP

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2439, BGP Route Flap Damping
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2004 - 2008 アライドテレシスホールディングス株式会社

PN: J613-M0021-12 Rev.L