[index] CentreCOM 8948XL コマンドリファレンス 2.9

# SHOW BGP AGGREGATE

カテゴリー：IP / 経路制御（BGP-4）
備考：フィーチャーライセンス AT-FL-09 が必要

`SHOW BGP AGGREGATE`

集約経路エントリーの一覧を表示する。

入力・出力・画面例

    Manager > show bgp aggregate

    BGP aggregate entries

    Prefix              Summary   Route map
    ----------------------------------------------
    192.168.0.0/19      Yes       -
    192.168.64.0/19     Yes       -
    ----------------------------------------------

表 1
Prefix | プレフィックス
Summary | 集約経路だけを通知するか（Yes）、個々の経路も通知するか（No）
Route map | 集約経路に適用するルートマップ名

関連コマンド

ADD BGP AGGREGATE
DELETE BGP AGGREGATE
SET BGP AGGREGATE
SHOW BGP ROUTE

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2439, BGP Route Flap Damping
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2004 - 2008 アライドテレシスホールディングス株式会社

PN: J613-M0021-12 Rev.L