[index] CentreCOM 8948XL コマンドリファレンス 2.9

# SET SNMP ENGINEID

カテゴリー：運用・管理 / SNMP

`SET SNMP ENGINEID=id`

id: SNMPエンジンID（5〜32バイトの16進数）

（SNMPv3）エンジンID（snmpEngineID）を変更する。
本コマンドを実行すると、定義済みのSNMPユーザーがすべて削除される（削除前に確認のプロンプトが出る）。

パラメーター

ENGINEID: SNMPエンジンID。5〜32バイトの16進数で指定する。すべて0の値、および、すべてFの値は使用できない。

備考・注意事項

通常はデフォルトのエンジンIDを使用すればよい。デフォルトのエンジンIDは長さ11オクテット（バイトと同義。以下はバイトとする）で、次のようにして生成される。
(1) 第1〜4バイトは、弊社のプライベート・エンタープライズ番号「000000CF」（16進。10進数では207）の第1バイトの先頭ビットを立てたもので、固定値「800000CF」となる。
(2) 第5バイトは固定値「03」（16進）で、これは後続の値がMACアドレスであることを示す。
(3) 第6〜11バイトはMACアドレス。

関連コマンド

SHOW SNMP

参考

RFC1157, A Simple Network Management Protocol (SNMP)
RFC1213, Management Information Base for Network Management of TCP/IP-based internets: MIB-II
RFC1901, Introduction to Community-based SNMPv2
RFC1902, Structure of Management Information for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1903, Textual Conventions for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1904, Conformance Statements for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1905, Protocol Operations for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1906, Transport Mappings for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1907, Management Information Base for Version 2 of the Simple Network Management Protocol (SNMPv2)

(C) 2004 - 2008 アライドテレシスホールディングス株式会社

PN: J613-M0021-12 Rev.L