IPマルチキャスト

サブカテゴリー別索引

概要

[A] [C] [D] [E] [P] [R] [S]

    A (top)

    ADD DVMRP INTERFACE
    ADD IGMP FILTER
    ADD IGMPSNOOPING ROUTERADDRESS
    ADD IP IGMP DESTINATION
    ADD PIM BSRCANDIDATE
    ADD PIM INTERFACE
    ADD PIM RPCANDIDATE

    C (top)

    CREATE IGMP FILTER
    CREATE IP IGMP DESTINATION

    D (top)

    DELETE DVMRP INTERFACE
    DELETE IGMP FILTER
    DELETE IGMPSNOOPING ROUTERADDRESS
    DELETE IP IGMP DESTINATION
    DELETE PIM BSRCANDIDATE
    DELETE PIM INTERFACE
    DELETE PIM RPCANDIDATE
    DESTROY IGMP FILTER
    DESTROY IP IGMP DESTINATION
    DISABLE DVMRP
    DISABLE DVMRP DEBUG
    DISABLE IGMPSNOOPING
    DISABLE IP IGMP
    DISABLE IP IGMP ALLGROUP
    DISABLE IP IGMP INTERFACE
    DISABLE PIM
    DISABLE PIM DEBUG

    E (top)

    ENABLE DVMRP
    ENABLE DVMRP DEBUG
    ENABLE IGMPSNOOPING
    ENABLE IP IGMP
    ENABLE IP IGMP ALLGROUP
    ENABLE IP IGMP INTERFACE
    ENABLE PIM
    ENABLE PIM DEBUG

    P (top)

    PURGE DVMRP
    PURGE PIM

    R (top)

    RESET DVMRP INTERFACE
    RESET PIM INTERFACE

    S (top)

    SET DVMRP INTERFACE
    SET IGMP FILTER
    SET IGMPSNOOPING ROUTERMODE
    SET IGMPSNOOPING VLAN FASTLEAVE
    SET IP IGMP
    SET PIM
    SET PIM BSRCANDIDATE
    SET PIM INTERFACE
    SET PIM LOG
    SET PIM RPCANDIDATE
    SHOW DVMRP
    SHOW IGMP FILTER
    SHOW IGMPSNOOPING
    SHOW IGMPSNOOPING ROUTERADDRESS
    SHOW IP IGMP
    SHOW PIM